Conexión
Usuario
Contraseña
English
Español
Français
Italiano
The Username/Password you entered is incorrect.....
Suomi
//10
System Identification
Option
Value
Description
Installation ID
Installation Name
Installer Name
Installer Phone
Display Installer
//20
Numeric identification of this installation, this is used in all reporting
to uniquely identify this installation ( 1-999999 )
Description of this installation
Name of installer for support purposes
Phone number of installer for support purposes
Check this setting if the installer details are to be displayed on keypads
Save


//30
Indentification
Standards
Options
Timers
Inputs
Outputs
Clock
Language

//40
New Installation
Back
System
Expanders
Wireless
Zones
Users
Help

//50
Standard compliance settings
Select for compliance to UK PD6662 requirements
Select for compliance to Irish Standards requirements
Select for compliance to European requirements
Select for Engineer configure
Grade 2
Grade 3
Grade

//60
None
Single
Dual






//70
Not Used
External Bell
Ext.Bell Strobe
Internal Bell
Alarm
Alarm Confirmed
Panic
Holdup
Fire
//80
Tamper
Medical
Fault
Technical
Mains Fault
Battery Fault
Partset A
Partset B
Full Set
//90
Fail To Set
Entry/Exit
Latch
Fire Exit
Chime
Smoke
Walktest


//100
Controller Inputs
Input
End Of Line
Analysed
Pulse Count (0-7)
Gross Attack (0-99)
Save


//110
System Options
Option
Value
Description
Areas
Check this setting if the system requires multiple areas.
Output Logging
Check this setting if logging is required for all outputs changing state.
Bell on First
//120
When this is checked, relevant external and internal Bell/Strobe outputs
will activate on an unconfirmed alarm. When not checked, bells will only
activate on a confirmed alarm, or if the detector that caused the
unconfirmed alarm is reactivated.
Bell Retrigger
If checked then the bells/sirens will resound if a second Zone activation
is detected after the Bell Time has elapsed. If not checked (default),
then the external bells will only trigger once.
PIN digits
//130
Number of digits in user codes.
Auto Restore
If checked then alerts will auto restore, if not checked then 
alerts require manual restore
Allow Engineer
If checked then a user must grant engineer access
Allow Manufacturer
If checked then a user must grant manufacturer access
System Alerts
//140
Configure system reactions to system alerts on keypads
Zone Alarm
Configure zone alarm options
Zone Tamper
Configure zone tamper options
Edit
Save


//150
None
Single 1K
Single 2K2
Single 4K7
Dual 1K/1K
Dual 2K2/2K2
Dual 4K7/2K2
PIR Masking

//160
Controller mains fault
Controller battery fault
Controller aux. fuse fault
Controller external bell fuse fault
Controller internal bell fuse fault
Controller bell tamper
Controller cabinet tamper
Controller aux. tamper 1
Controller aux. tamper 2
//170
Controller antenna tamper
Controller RF Jamming
Modem 1 fault
Modem 1 line fault
Modem 2 fault
Modem 2 line fault
E-BUS cable fault
E-BUS expander communication fault
E-BUS expander mains fault
//180
E-BUS expander fuse fault
E-BUS expander battery fault
E-BUS expander rf jamming
E-BUS expander cabinet tamper
E-BUS expander antenna tamper




//190
Alarm
Entry/Exit
Exit Term
Fire
Fire Exit
Line
Panic
Holdup
Tamper
//200
Tech
Medical
Unused






//210
Settings
Receiver 1
Receiver 2
Receiver 3
Receiver 4




//220
Status
Log
Intruder Settings
Comm. Settings
Advanced
Help



//230
AT   AC Trouble
AR   AC Restoral
BA   Burglary Alarm
BB   Burglary Bypass
BC   Burglary Cancel
BD   Swinger Trouble
BE   Swinger Trouble Restore
BJ   Burglary Trouble Restore
BR   Burglary Restoral
BT   Burglary Trouble
BU   Burglary Unbypass
BV   Burglary Verified
BX   Burglary Test
CD   Closing Delinquent
CF   Forced Closing
CG   Close Area
CI   Fail to Close
CL   Closing Report
CP   Automatic Closing
CQ   Remote Closing
CS   Closing Keyswitch
EA   Exit Alarm
EJ   Expansion Tamper Restore
ES   Expansion Device Tamper
FA   Fire Alarm
FB   Fire Bypass
FC   Fire Cancel
FJ   Fire Trouble Restore
FR   Fire Restoral
FT   Fire Trouble
FU   Fire Unbypass
HA   Holdup Alarm
HB   Holdup Bypass
HJ   Holdup Trouble Restore
HR   Holdup Restoral
HT   Holdup Trouble
HU   Holdup Unbypass
JA   User Code Tamper
JT   Time Changed
LB   Local Programming
LR   Phone Line Restoral
LT   Phone Line Trouble
LX   Local Programming Ended
MA   Medical Alarm
MB   Medical Bypass
MJ   Medical Trouble Restore
MR   Medical Restoral
MT   Medical Trouble
MU   Medical Unbypass
NL   Perimeter Armed
NR   IP Link Restore
NT   IP Link Fail
OA   Automatic Opening
OG   Open Area
OP   Opening Report
OQ   Remote Opening
OR   Disarm From Alarm
PA   Panic Alarm
PB   Panic Bypass
PJ   Panic Trouble Restore
PR   Panic Restoral
PT   Panic Trouble
PU   Panic Unbypass
RC   Relay Close
RN   Remote Reset
RO   Relay Open
RR   Power up
RS   Remote Program Success
RT   Data Lost
RX   Manual Test
TA   Tamper
TB   Tamper Bypass
TR   Tamper Restoral
TU   Tamper Unbypass
TX   Test call
UA   Untyped Alarm
UB   Untyped Bypass
UJ   Untyped Trouble Restore
UR   Untyped Restoral
UT   Untyped Trouble
UU   Untyped Unbypass
YA   Bell Fault
YC   Communication Fail
YF   Checksum Fault
YH   Bell Restored
YK   Communication Restoral
YM   Battery Missing
YP   PSU Trouble
YQ   PSU Restoral
YR   Battery Restoral
YS   Communication Trouble
YT   Battery Trouble
YW   Watchdog Reset
YX   Service Required
YZ   Service Completed




//330
Output Trigger
Zone Trigger
Time Trigger
OPEN
CLOSE
ON
OFF


//340
Add New X10 Trigger
Trigger Type
Output:
State:
Add




//350
Advanced - X10
X10 Device Trigger
Unit
Active
Description
Trigger ON
Trigger OFF
RKD
Save
//360
Area Configuration
Area Edit
Area
Active
Description
Entry Time
Exit Time
Seconds
This Area is a common area for the following Areas:
//370
SIA
Contact ID
Fast Format
Primary
Backup
Comms. Settings - ARC
Add Alarm Receiving Centre
Description
Account
//380
Protocol
Priority
Number 1
Number 2
Indentification of Alarm Receiving Centre
Account Number
Protocol used in communication
Priority of ARC
Phone number 1
//390
Phone number 2
Save
Central Station
None
Comm. Settings - EDP
EDP Settings
Device ID
Event Timeout
Retry Count
//400
Dial Attempts
Dial Delay
Dial Lockout
Unique Identification of this device
Number of seconds between retransmissions of unacknowledged events
Max number of retransmissions (5-199)
Max number of failed dial attempts before Modem lockout (1-199)
Seconds to wait before redialing after a failed dial attempt (1-199)
Seconds to suspend dialling when max number of failed dial attempts are reached
//410
Save
Receiver 1 Settings
Receiver 2 Settings
Receiver 3 Settings
Receiver 4 Settings
Receiver 1 Event Filter
Receiver 2 Event Filter
Receiver 3 Event Filter
Receiver 4 Event Filter
//420
Unique ID
Name
Encyrption Enabled
Encryption Key
Network Settings
IP Address
IP Port
Polling Enabled
IP Polling Interval
//430
IP Poll Fail Trigger
Modem Settings
Modem Number
Modem Test Enabled
Test Interval 1
Test Interval 2
Event Settings
Reporting Enabled
Primary Receiver
//440
IP Enable
Modem Enable
Backup
Command Settings
Commands Enable
32 Hex Digits
UDP port for receiving data
Select this to enable IP polling from this receiver
Seconds between IP polls (1 - 9999)
//450
Number of missing polls before network fail is registered
Phone number to dial
Automatic modem test calls
Minutes between test calls when network link is up
Minutes between test calls when network link is down
Check if events should be reported to this receiver
Check if primary, clear for backup
Check if events can be reported through IP
Check if events can be reported through Modem
//460
Choose backup receiver
Check if incoming commands are allowed from this receiver
Configured Alarm Reporting Centres
ARC
Account
Protocol
Priority
Number 1
Number 2
//470
Comms. Settings - Modem
Modem Settings
Modem
Type
Status
Answer Incoming
PIN Code


//480
Comms. Settings - Network
Ethernet Settings
IP Address
IP Network
Gateway IP Address
DHCP Enabled
EDP Port
Select this to use Dynamic Address
IP Port for receiving EDP data over network (Europlex Datagram Protocol)
//490
Save
Network Services
HTTP Enabled
HTTP Port
Telnet Enabled
Telnet Port
ENMP Enabled
ENMP Port
ENMP Update Enabled
//500
ENMP Change Password
Select this to enable web server
Port web server is listening on
Select this to enable telnet server
Port telnet server is listening on
Select this to enable Europlex Network Management Protocol
Port ENMP is listening on
Select this to enable network config changes through ENMP
Password for ENMP config changes
//510
Comms. Settings - Serial
Serial Port Configuration
Serial Port :
Type :
Bits per Second :
Data Bits :
Parity :
Stop Bits :
Flow Control :
//520
X10
Terminal
Printer
Int.Modem
Ext.Modem
Terminal
Printer


//530
Add New Account
Account Name
Add New Account






//540
Connection
Select Comms Path:
Connect to
IP Connection
Direct (Serial/USB)
Modem 1
Modem 2
Connect

//550
Edit Installation
Installation ID :
Installation Name :
Installation Address :
Panel Type :
Account :
IP Address :
Telephone Number 1 :
Telephone Number 2 :
//560
Add/Edit Accounts
Save New Configuration
Event Filter
Select/Clear All
Save




//570
Save SigNET Installation Details
Installation Details :
Installation ID :
N.B. Must be unique ID (1-9999)
Installation Name :
Istallation Address :
Panel Type :
Account :
IP Address :
//580
Telephone Number 1 :
Telephone Number 2 :
Cancel
Save
Add/Edit Accounts
ID
Installation Name
Address
Panel Type
//590
Account
Modified Date
SigNET Installations
Account Filter :
Cancelación
Corregir
Trabajo fuera de línea
Trabajo en línea

//600
Import from Flash
Export to Flash
Installation Details
SigNET
System Summary
IP Address :
Installation ID :
Installation Name :
Installer Name :
//610
Installer Phone :
Last Downloaded to Panel :
Last Uploaded from Panel :
Area Configuration
Area
Active 
Text
Entry
Exit
//620
Common
Save
Intruder Settings - Expanders
Configured Expanders
Expander
Status
Type
Serial#
Description
//630
Inputs
Outputs
Save
Intruder Settings - Users
User  Configuration
User
Name
Level
Rights
//640
Time Limit
Date Limit
Save
Intruder Settings - Zones
Zone Configuration
Zone
Active
Input
Zone Text
//650
Type
Area
Attributes
Save
Policy Settings
USER OPTIONS
ENGINEER OPTIONS
SYSTEM
Alert
//660
Restore
Inhibit
Isolate
Restore
Inhibit
Isolate
Alarm
Arming
Save
//670
Limited
Standard
Manager
Unset
Partset A
Partset B
Full Set
Restore
Inhibit
//680
Bell Test
Chime
Walktest
Set Date
View Log
Users
Engineer
Upgrade
Web Access
//690
X-10
Change Code
Force Set
SMS
<Unused>
Configure Panel User
Configure User
User :
User Name :
//700
User Code :
Level :
Panel Rights for this user :
Areas this user has access to :
Time Restriction
Date Restriction
Enable Restriction
From :
To :
//710
Hr
Mn
Save
X-10 Triggers
X-10 ON Triggers :
X-10 OFF Triggers :
Device Type
Device State
Device Name / Time
//720
Add
Delete
Close
Zone Configuration
Zone Edit
Zone :
Active :
Description :
Input :
//730
Type :
Area :
Attributes :
Save
Language
File
Help
Import Installation from File
Export Installation to File
//740
Read from USB Flash Programmer
Write to USB Flash Programmer
Exit
Contents
About




//750
Installation Setup/Listing
Exit Config. Mode
Back
Network
Serial
Modem
ARC
EDP
Areas
//760
X-10
File
Show All Installations
Add New Installation
Summary
Zones
System Alerts
EBUS
List
//770
AutoConfigure
Ethernet
Services
List
Add
Settings
Triggers


//780
Output
Zone
Timer
X-10 Settings
Enable:
X-10 Controller
Log:
Check to enable X-10
Check to log X-10 commands
//790
Select X-10 controller type connected to SigNET X-10 serial port
Language
Delete Installation
ID
Are you sure?
Are you sure you wish to exit Config Mode?
System Timers
Timer
Value
//800
Description
Internal Bells
External Bells
External Bell Strobe
External Bell Delay
Chime
Confirm
Double Knock
Soak
//810
RKD Timeout
Entry
Exit
Duration that internal sounders will sound when alarm is activated.
Duration that external sounders will sound when alarm is activated.
Duration that strobe output will be active when alarm is activated, 0 = Forever. 
Delayed activation of external sounders.
Max time between alarms from 2 non-overlapping zones, 
that will cause a confirmed alarm. (Minutes)
//820



The number of seconds allowed to enter premises during unsetting
The number of seconds allowed to leave premises during setting
Save
Controller Outputs
Output
Text
//830
Type
Negative
Save
Language Option
Language
Select language used on keypads, web interface, and reporting of events
Save
<Assigned>

//840
None
Even
Odd
Off
Not Fitted
Enabled
SIA Code

Event Filter for Receiver
//850
Receiver
Event
All Groups
Installation ID
There is no file associated with this installation...
You need to connect to the panel and upload the current configuration 
to allow offline editing....
Config File Warning!
Installation
//860
Area
<Not Assignable>
<Assigned as Common>
Controller
Input
Expander
ON
OFF
OPEN
//870
CLOSE
Time
Zone
Online
(Minutes)
(Seconds)
Duration Chime output will activate, when a zone with CHIME attribute opens.
Max delay between activations of zones with the double attribute 
which will cause an alarm. (Seconds)
//880
Number of days a zone remains under soak test before 
returning to normal operation. (Days)
Number of seconds that an RKD will wait for key entry before it leaves 
the current menu. (Seconds)
DEFAULT GROUP
Are you sure you want to delete the selected trigger?