Login
User
Password
English
Español
Français
Italiano
The Password you entered is incorrect.....
Suomi
//10
System Identification
Option
Value
Description
Installation ID
Installation Name
Installer Name
Installer Phone
Display Installer
//20
Numeric identification of this installation, this is used in all reporting
to uniquely identify this installation ( 1-999999 )
Description of this installation
Name of installer for support purposes
Phone number of installer for support purposes
Check this setting if the installer details are to be displayed on keypads
Save


//30
Indentification
Standards
Options
Timers
Inputs
Outputs
Clock
Language

//40
New Installation
Back
System
Expanders
Wireless
Zones
Users
Help

//50
Standard compliance settings
Select for compliance to UK PD6662 requirements
Select for compliance to Irish Standards requirements
Select for compliance to European requirements
Select for Unrestricted
Grade 2
Grade 3
Grade

//60
None
Single
Dual






//70
Not Used
External Bell
Ext.Bell Strobe
Internal Bell
Alarm
Alarm Confirmed
Panic
Holdup
Fire
//80
Tamper
Medical
Fault
Technical
Mains Fault
Battery Fault
Partset A
Partset B
Full Set
//90
Fail To Set
Entry/Exit
Latch
Fire Exit
Chime
Smoke
Walktest


//100
Controller Inputs
Input
End Of Line
Analysed
Pulse Count
Gross Attack
Save


//110
System Options
Option
Value
Description
Areas
Check this setting if the system requires multiple areas.
Output Logging
Check this setting if logging is required for all outputs changing state.
Bell on First
//120
When this is checked, relevant external and internal Bell/Strobe outputs
will activate on an unconfirmed alarm. When not checked, bells will only
activate on a confirmed alarm, or if the detector that caused the
unconfirmed alarm is reactivated.
Bell Retrigger
If checked then the bells/sirens will resound if a second Zone activation
is detected after the Bell Time has elapsed. If not checked (default),
then the external bells will only trigger once.
PIN digits
//130
Number of digits in user codes.
Auto Restore
If checked then alerts will auto restore, if not checked then 
alerts require manual restore
Allow Engineer
If checked then a user must grant engineer access
Allow Manufacturer
If checked then a user must grant manufacturer access
System Alerts
//140
Configure system reactions to system alerts on keypads
Zone Alarm
Configure zone alarm options
Zone Tamper
Configure zone tamper options
Edit
Save


//150
None
Single 1K
Single 2K2
Single 4K7
Dual 1K/1K
Dual 2K2/2K2
Dual 4K7/2K2
PIR Masking

//160
Controller mains fault
Controller battery fault
Controller aux. fuse fault
Controller external bell fuse fault
Controller internal bell fuse fault
Controller bell tamper
Controller cabinet tamper
Controller aux. tamper 1
Controller aux. tamper 2
//170
Controller antenna tamper
Controller RF Jamming
Modem 1 fault
Modem 1 line fault
Modem 2 fault
Modem 2 line fault
X-BUS cable fault
X-BUS expander communication fault
X-BUS expander mains fault
//180
X-BUS expander fuse fault
X-BUS expander battery fault
X-BUS expander rf jamming
X-BUS expander cabinet tamper
X-BUS expander antenna tamper




//190
Alarm
Entry/Exit
Exit Term
Fire
Fire Exit
Line
Panic
Holdup
Tamper
//200
Tech
Medical
Unused






//210
Settings
Receiver 1
Receiver 2
Receiver 3
Receiver 4




//220
Status
Log
Intruder Settings
Comm. Settings
Advanced
Help



//230
AT   AC Trouble
AR   AC Restoral
BA   Burglary Alarm
BB   Burglary Bypass
BC   Burglary Cancel
BD   Swinger Trouble
BE   Swinger Trouble Restore
BJ   Burglary Trouble Restore
BR   Burglary Restoral
BT   Burglary Trouble
BU   Burglary Unbypass
BV   Burglary Verified
BX   Burglary Test
CD   Closing Delinquent
CF   Forced Closing
CG   Close Area
CI   Fail to Close
CL   Closing Report
CP   Automatic Closing
CQ   Remote Closing
CS   Closing Keyswitch
EA   Exit Alarm
EJ   Expansion Tamper Restore
ES   Expansion Device Tamper
FA   Fire Alarm
FB   Fire Bypass
FC   Fire Cancel
FJ   Fire Trouble Restore
FR   Fire Restoral
FT   Fire Trouble
FU   Fire Unbypass
HA   Holdup Alarm
HB   Holdup Bypass
HJ   Holdup Trouble Restore
HR   Holdup Restoral
HT   Holdup Trouble
HU   Holdup Unbypass
JA   User Code Tamper
JT   Time Changed
LB   Local Programming
LR   Phone Line Restoral
LT   Phone Line Trouble
LX   Local Programming Ended
MA   Medical Alarm
MB   Medical Bypass
MJ   Medical Trouble Restore
MR   Medical Restoral
MT   Medical Trouble
MU   Medical Unbypass
NL   Perimeter Armed
NR   IP Link Restore
NT   IP Link Fail
OA   Automatic Opening
OG   Open Area
OP   Opening Report
OQ   Remote Opening
OR   Disarm From Alarm
PA   Panic Alarm
PB   Panic Bypass
PJ   Panic Trouble Restore
PR   Panic Restoral
PT   Panic Trouble
PU   Panic Unbypass
RC   Relay Close
RN   Remote Reset
RO   Relay Open
RR   Power up
RS   Remote Program Success
RT   Data Lost
RX   Manual Test
TA   Tamper
TB   Tamper Bypass
TR   Tamper Restoral
TU   Tamper Unbypass
TX   Test call
UA   Untyped Alarm
UB   Untyped Bypass
UJ   Untyped Trouble Restore
UR   Untyped Restoral
UT   Untyped Trouble
UU   Untyped Unbypass
YA   Bell Fault
YC   Communication Fail
YF   Checksum Fault
YH   Bell Restored
YK   Communication Restoral
YM   Battery Missing
YP   PSU Trouble
YQ   PSU Restoral
YR   Battery Restoral
YS   Communication Trouble
YT   Battery Trouble
YW   Watchdog Reset
YX   Service Required
YZ   Service Completed




//330
Output Trigger
Zone Trigger
Time Trigger
OPEN
CLOSE
ON
OFF


//340
Add New X10 Trigger
Trigger Type
Output:
State:
Add




//350
Advanced - X10
X10 Device Trigger
Unit
Active
Description
Trigger ON
Trigger OFF
RKD
Save
//360
Area Configuration
Area Edit
Area
Active
Description
Entry Time
Exit Time
Seconds
This Area is a common area for the following Areas:
//370
SIA
Contact ID
Fast Format
Primary
Backup
Comms. Settings - ARC
Add Alarm Receiving Centre
Description
Account
//380
Protocol
Priority
Number 1
Number 2
Indentification of Alarm Receiving Centre
Account Number
Protocol used in communication
Priority of ARC
Phone number 1
//390
Phone number 2
Save
Central Station
None
Comm. Settings - EDP
EDP Settings
Device ID
Event Timeout
Retry Count
//400
Dial Attempts
Dial Delay
Dial Lockout
Unique Identification of this device
Number of seconds between retransmissions of unacknowledged events
Max number of retransmissions (5-199)
Max number of failed dial attempts before Modem lockout (1-199)
Seconds to wait before redialing after a failed dial attempt (1-199)
Seconds to suspend dialling when max number of failed dial attempts are reached
//410
Save
Receiver 1 Settings
Receiver 2 Settings
Receiver 3 Settings
Receiver 4 Settings
Receiver 1 Event Filter
Receiver 2 Event Filter
Receiver 3 Event Filter
Receiver 4 Event Filter
//420
Unique ID
Name
Encyrption Enabled
Encryption Key
Network Settings
IP Address
IP Port
Polling Enabled
IP Polling Interval
//430
IP Poll Fail Trigger
Modem Settings
Modem Number
Modem Test Enabled
Test Interval 1
Test Interval 2
Event Settings
Reporting Enabled
Primary Receiver
//440
IP Enable
Modem Enable
Backup
Command Settings
Commands Enable
32 Hex Digits
UDP port for receiving data
Select this to enable IP polling from this receiver
Seconds between IP polls (1 - 9999)
//450
Number of missing polls before network fail is registered
Phone number to dial
Automatic modem test calls
Minutes between test calls when network link is up
Minutes between test calls when network link is down
Check if events should be reported to this receiver
Check if primary, clear for backup
Check if events can be reported through IP
Check if events can be reported through Modem
//460
Choose backup receiver
Check if incoming commands are allowed from this receiver
Configured Alarm Reporting Centres
ARC
Account
Protocol
Priority
Number 1
Number 2
//470
Comms. Settings - Modem
Modem Settings
Modem
Type
Status
Answer Incoming
PIN Code


//480
Comms. Settings - Network
Ethernet Settings
IP Address
IP Network
Gateway IP Address
DHCP Enabled
EDP Port
Select this to use Dynamic Address
IP Port for receiving EDP data over network (Enhanced Datagram Protocol)
//490
Save
Network Services
HTTP Enabled
HTTP Port
Telnet Enabled
Telnet Port
ENMP Enabled
ENMP Port
ENMP Update Enabled
//500
ENMP Change Password
Select this to enable web server
Port web server is listening on
Select this to enable telnet server
Port telnet server is listening on
Select this to enable Enhanced Network Management Protocol
Port ENMP is listening on
Select this to enable network config changes through ENMP
Password for ENMP config changes
//510
Comms. Settings - Serial
Serial Port Configuration
Serial Port :
Type :
Bits per Second :
Data Bits :
Parity :
Stop Bits :
Flow Control :
//520
X10
Terminal
Printer
Int.Modem
Ext.Modem
Terminal
Printer


//530
Add New Group
Group Name
Add New Group






//540
Connection
Select Comms Path:
Connect to
IP Connection
Direct (Serial/USB)
Modem 1
Modem 2
Connect

//550
Edit Installation
Installation ID :
Installation Name :
Installation Address :
Panel Type :
Group :
IP Address :
Telephone Number 1 :
Telephone Number 2 :
//560
Add/Edit Group
Save New Configuration
Event Filter
Select/Clear All
Save




//570
Save SPC Installation Details
Installation Details :
Installation ID :
N.B. Must be unique ID (1-999999)
Installation Name :
Installation Address :
Panel Type :
Group :
IP Address :
//580
Telephone Number 1 :
Telephone Number 2 :
Cancel
Save
Add/Edit Accounts
ID
Installation Name
Address
Panel Type
//590
Group
Modified Date
SPC Installations
Account Filter :
Delete
Edit
Work Offline
Work Online

//600
Import from Flash
Export to Flash
Installation Details
SPC
System Summary
IP Address :
Installation ID :
Installation Name :
Installer Name :
//610
Installer Phone :
Last Downloaded to Panel :
Last Uploaded from Panel :
Area Configuration
Area
Active 
Text
Entry
Exit
//620
Common
Save
Intruder Settings - Expanders
Configured Expanders
Expander
Status
Type
Serial#
Description
//630
Inputs
Outputs
Save
Intruder Settings - Users
User  Configuration
User
Name
Level
Rights
//640
Time Limit
Date Limit
Save
Intruder Settings - Zones
Zone Configuration
Zone
Active
Input
Zone Text
//650
Type
Area
Attributes
Save
Policy Settings
USER OPTIONS
ENGINEER OPTIONS
SYSTEM
Alert
//660
Restore
Inhibit
Isolate
Restore
Inhibit
Isolate
Alarm
Arming
Save
//670
Limited
Standard
Manager
Unset
Partset A
Partset B
Full Set
Restore
Inhibit
//680
Bell Test
Chime
Walktest
Set Date
View Log
Users
Engineer
Upgrade
Web Access
//690
X-10
Change Code
Force Set
SMS
<Unused>
Configure Panel User
Configure User
User :
User Name :
//700
User Code :
Level :
Panel Rights for this user :
Areas this user has access to :
Time Restriction
Date Restriction
Enable Restriction
From :
To :
//710
Hr
Mn
Save
X-10 Triggers
X-10 ON Triggers :
X-10 OFF Triggers :
Device Type
Device State
Device Name / Time
//720
Add
Delete
Close
Zone Configuration
Zone Edit
Zone :
Active :
Description :
Input :
//730
Type :
Area :
Attributes :
Save
Language
File
Help
Import Installation from File
Export Installation to File
//740
Read from USB Flash Programmer
Write to USB Flash Programmer
Exit
Contents
About




//750
Installation Setup/Listing
Exit Config. Mode
Back
Network
Serial
Modem
ARC
EDP
Areas
//760
X-10
File
Show All Installations
Add New Installation
Summary
Zones
System Alerts
X-BUS
List
//770
AutoConfigure
Ethernet
Services
List
Add
Settings
Triggers


//780
Output
Zone
Timer
X-10 Settings
Enable:
X-10 Controller
Log:
Check to enable X-10
Check to log X-10 commands
//790
Select X-10 controller type connected to SPC X-10 serial port
Language
Delete Installation
ID
Are you sure?
Are you sure you wish to exit Config Mode?
System Timers
Timer
Value
//800
Description
Internal Bells
External Bells
External Bell Strobe
External Bell Delay
Chime
Confirm
Double Knock
Soak
//810
RKD Timeout
Entry
Exit
Duration that internal sounders will sound when alarm is activated.
Duration that external sounders will sound when alarm is activated.
Duration that strobe output will be active when alarm is activated, 0 = Forever. 
Delayed activation of external sounders.
Max time between alarms from 2 non-overlapping zones, 
that will cause a confirmed alarm. (Minutes)
//820



The number of seconds allowed to enter premises during unsetting
The number of seconds allowed to leave premises during setting
Save
Controller Outputs
Output
Text
//830
Type
Negative
Save
Language Option
Language
Select language used on keypads, web interface, and reporting of events
Save
<Assigned>

//840
None
Even
Odd
Off
Not Fitted
Enabled
SIA Code

Event Filter for Receiver
//850
Receiver
Event
All Groups
Installation ID
There is no file associated with this installation...
You need to connect to the panel and upload the current configuration 
to allow offline editing....
Config File Warning!
Installation
//860
Area
<Not Assignable>
<Assigned as Common>
Controller
Input
Expander
ON
OFF
OPEN
//870
CLOSE
Time
Zone
Online
(Minutes)
(Seconds)
Duration Chime output will activate, when a zone with CHIME attribute opens.
Max delay between activations of zones with the double attribute 
which will cause an alarm. (Seconds)
//880
Number of days a zone remains under soak test before 
returning to normal operation. (Days)
Number of seconds that an RKD will wait for key entry before it leaves 
the current menu. (Seconds)
DEFAULT GROUP
Are you sure you want to delete the selected trigger?



//890
Options
Advanced
Change Login Password
System Options
Firmware Upgrade (Full Engineer Mode Only)
Group
Date Stamp
IP
Modem
//900
SPC Fast Programmer
Add New
Configure
Add/Edit Installation Groups
SPC Pro Installations
Installations may be filtered by Group using the drop-down list below....



//910
About
Version
Warning: This computer program is protected by copyright law and international treaties.
Unauthorised reproduction or distribution of this program may result in civil 
and criminal penalties.
Compatible with the following panel types:
Delete Installation
Edit Installation Details
Configure Installation
//920  '-- Wireless Detector Types
Unknown
Magnetic Contact
Inertia
PIR
Universal
Smoke Detector
Flood Detector
Gas Detector
Panic Button
CO Detector
Handheld


Keyarm
Shunt
X-Shunt



//940  '-- Node Types
Keypad
I/O Expander
I/O Analysed
PSU
Wireless
Unknown Type



//950
Export configuration to file...
SPC Config Format
Export for
SPC Config Files
Select SPC config file to import to SPC Pro...
Restarting panel... Please Wait....
Receiving Config File
Reading Outputs Status....
Retrieving new Datestamp info.... 
//960
General
Panel Status
View panel details and status.
View Log
View the historical panel log.
Setup Users
View/Edit/Add panel users.
X-10 Config
Configure X10 and triggers.
//970
Panel Settings
System Settings
Engineer setup, Options, etc....
Controller Inputs & Outputs
Modify the Controller inputs and outputs....
Expanders & Keypads
Modify or Add new expanders to the system
Wireless
View wireless detectors configured on the system
//980
All Zones
Configure zones on the system
Communications
Serial Ports
Modem Configuration
Alarm Reporting Centres
EDP Setup


//990
Please exit Config Mode before exiting program.....
Configuration has been exported to file location :
Problem occurred opening
file
Please make sure you have the Acrobat Reader installed...
Cannot find
Last command to SPC timed out!!
Problem Compressing the file - Configuration not sent to panel!!!
Failed to uncompress config file...
//1000
Failed to retrieve config file from panel... 
Function only available when online with panel....
Error decrypting the config file!!!
Problem Compressing the file - Configuration not sent to panel!!!
Save all changes made?
Save & Send config file to panel?
Download config file from panel? 
This will overwrite all changes you have made in SPC Pro....
Some changes have not yet been saved.... Save now to file?
//1010
Do you wish to download the configuration to the online panel?
File already exists - Overwrite?
Confirm
Problem occurred while compressing the file!... 
Areas
Configure Areas on the panel.
Holidays
Configure Holidays on the panel.

//1020
Auto Arming
Configure Auto Arming on the panel.
Network Settings
Configure network settings and services.
EDP Setup
Configure EDP Settings.



//1030
www.siemens.com
SPC Pro Panel Config Application
siemens
SPC Pro
OK
Connect to Fast Programmer...
Fast Programmer
Select
Connect
//1040
Could not detect a SPC Fast Programmer!
Fast Programmer Manager
Files found on Fast Programmer
Port
Version
Warning : Do not unplug the Fast Programmer while the 'Fast Programmer 
Manager' form is open....
Refresh
Delete All Files
//1050
Delete File
Close
Import from Programmer
Export to Programmer
% Used Space
% Free Space
Capacity
Bytes

//1060
ID
FileName
Size (Bytes)
Date
Updating file list...
Import file from Fast Programmer:
Receiving file from Programmer....
Export file to Fast Programmer:

//1070
Delete file
from Programmer?
Problem occurred trying to delete the file!!
Delete all files from Programmer?
Import file
Select a file to import!
This is a Log file.
SPC Pro will extract and open this file in Notepad.
Continue?
//1080
Import Config File
Error decrypting the config file!!!
Problem occurred getting file from programmer!!
Problem occurred trying to delete the files!!
Please select a file to Import....




//1090
Programmer File Export
Select Installation to Export
Filename on Programmer
Progress
Export
Choose Installation....
Please enter a valid file name....
There is not enough free space on the Fast Programmer 
to complete this request!...
//1100
File name already exists on the programmer!
Do you wish to overwrite?
Exporting File...
Refreshing....
Please Wait......
Warning
Add EDP Receiver
Configuration details for new EDP receiver....
Description
//1110
Receiver ID
Network Address
Phone Number 1
Phone Number 2
Description of receiver
Unique identification number.
IP address of receiver. (Leave blank if dial-up only)
Phone number of receiver. (Leave blank if IP only)
Backup phone number of receiver. (Leave blank if IP only)
//1120
OK
Cancel
Please enter a Receiver ID before saving....
You already have a Receiver entry with this Receiver ID!...
Add Expander
Add New Expander
Select Expander type details
Expander ID
Serial #
//1130
Description
Type
Input
Output
Maximum number of expanders has been reached!...
Maximum number of keypads has been reached!...
Maximum number of I/O Expanders has been reached!...


//1140    'Zone Attributes
Access
Exclude A
Exclude B
24 Hour
Local
Double Knock
Chime
Inhibit
Normally Open
Silent
Log
Open Only
Report Only
Final Exit
Keyarm Fullset
Keyarm Unset
Shunt


//1160  'Output Types
Autoarm
User Duress
PIR Masked
Zones Omitted





//1170
January
February
March
April
May
June
July
August
September
//1180
October
November
December

Zone Config
Edit the zone details....
OK
Cancel

//1190
Please select valid zone type from list...
Edit Groups
Edit Installation Groups
Delete
Add New
Rename
Close
Group Description
You cannot delete the default group!...
//1200
Please select a group from the list...
Delete group
Installations in this group will be reassigned to the 'DEFAULT' group....
Change Login Parameters
Change Login Password
Old Login Password
New Login Password
Confirm New Password
Save
//1210
Cancel
Please enter a new login password!...
New and Confirmed codes do not match!
Login password has been changed...
You must download the config file for change to take affect at panel...
Old password is incorrect!!



//1220
System Options
General
Modem Options
Check config file datestamp on panel connect...
Predial String
Wait Time
1-60 sec
OK
Cancel
//1230
Add X-10 ON Trigger
Add X-10 OFF Trigger
Trigger Type
Trigger
Output Trigger
Zone Trigger
Time Trigger
Wireless FOB
Hour
//1240
Minute
Zone
State
User Fob
Cancel
User
File selected is not a valid SPC Firmware file.....


//1250
Firmware Upgrade
Selected Firmware File Details....
File Path:
Firmware Type
Panel Type
Firmware Version
Length
CRC
Upgrade Now...
//1260
Cancel
N.B. : After you send the firmware file the panel will restart.
You will lose connection and will need to reconnect
once the panel has fully rebooted....
Firmware Updated!....
Firmware update successful... SPC Pro will now disconnect...
NOTE: You must unplug and reinsert the USB cable to the panel
 before reconnection is possible!
Warning: Once upgrade procedure has started you cannot cancel... Continue?
//1270
Direct - USB
Direct - Serial RS232
Comport :
Receiving File....
Cancel....
No SPC comport detected!...
Connect
Retrieving Device info.... 

//1280
The firmware on this panel has features not supported by this
version of SPC Pro.... 
You need to install the latest version of SPC Pro to connect to this panel....
The firmware in this panel is not supported by SPC Pro....
Please upgrade your SPC panel firmware before reconnecting....
Current Firmware version in panel
Firmware Version Issue
Connect anyway?

//1290
You are connected to a
The config file stored on disk is incorrect... Continue?
Could not detect a SPC panel on selected port..
Could not detect a valid SPC panel....
SPC Pro has detected that the config file in the panel
may not be in synch with the config file on the PC:
Panel config file datestamp
PC config file datestamp

//1300
It is recommended that you perform a file upload or download
to synchronise config files.
Retrieving Status info.... 
No SPC panel connected on USB!
Please select a connection path!....
Loading Installation Configuration file.....
INSTALLATION
Please make a selection from the Installations list...
Please enter a valid Installation ID!....
//1310
You already have an installation with that ID
please change the Installation ID
Do you wish to send config file for ID
Output Trigger
Zone Trigger
Time Trigger
Wireless Fob Trigger


//1320
Add triggers and details....
Enabled
Description
X-10 Keypad
Test X-10 Device -
OFF
ON
OK
Cancel
//1330
Wireless FOB
User FOB
Zone
User
Sending Command to turn X10 Device
None
Triggers for X-10 Device
Settings
X-10 Device Triggers
//1340
General - X10 Config
Connect To Panel
Disconnect from Panel
Send Config File to Panel
Get Config File from Panel
Keypad Emulation
Toggle Engineer Mode
Configuration Summary Printout
Save Config File Changes
//1350
Exit Config Mode
Config Mode Toolbar
ONLINE
Offline
Retrieving new Datestamp info.... 
Receiving Config file....
Refreshing Configuration data...
Activating Soft Engineer Mode... 
Activating Full Engineer Mode... 
//1360
Problem Compressing the file - Configuration not sent to panel!!!
Failed to uncompress config file...
Save all Config File changes made?
Disconnect from panel?
Save Changes & Send Config File to panel?
Get config file from panel?
Configure User
Edit Rights, Areas, Restrictions, etc...
SMS Setup
//1370
Enable
Number
Events
Check to enable engineer to receive SMS events
Alarm Activation
Alarms confirmed by multiple zones
Fault and Tamper activations
Arming and Disarming
Inhibit and Isolate
//1380
All other types of events
OK
Delete
Cancel
Please select a different user code...
Are you sure you wish to delete User
RFID Tag
Wireless FOB
Add User
//1390
Change Engineer Code
Engineer SMS Message Setup
Engineer Web Code
All Users
General - Setup Users
Isolate
Delay Autoarm


//1400
Panel Log
General - Panel Log
System Log
From
To
Date
Time
Get Log
Save Log to File
//1410
Log
Text Format
Requesting Log File....
Start date must be earlier than end date!!....
Please connect to panel before running report....
File already exists - Overwrite?
Logfile for
Confirm

//1420
Select Soft Engineer Mode
Select Full Engineer Mode
Engineer Code
Change Engineer Code
PIN Code
Old Code
New Code
Confirm New Code
OK
//1430
Cancel
N.B. Change will not take effect until the config file has been sent to the panel....
Web Access Code
Web Code Enable
Leave unchecked to use PIN code for web access
Engineer PIN code changed!
You must download the config file for change to take affect at panel...
New and Confirmed PIN codes do not match!
Old engineer code incorrect!...
//1440
Engineer Web code changed!
New and Confirmed Web Codes do not match
Please enter a valid Web Code....
SMS Setup
Engineer SMS Setup
OK
Cancel
Panel Settings - Zones
List
//1450
Wireless Sensor
Panel Settings - Wireless
Wireless Sensors
Remove Wireless Sensors
View Sensor Log
Show Unenrolled Wireless Devices
List
Settings

//1460
Internal
External
Tamper Disabled
Tamper Enabled
Wireless Settings
Antenna
Select which type of antenna is connected to the wireless module.
Supervision
Select whether missing supervision for a sensor will raise a zone tamper.
//1470
OK
Requesting event log for Sensor ID
Quick Log - Sensor ID
No Wireless device selected!...
Please select a Wireless Sensor from the grid...
Do you wish to delete Sensor ID



//1480
Sensor
ID
Type
Zone
Battery
Supervise
Unenrolled Devices
Unenrolled Wireless Devices
Select a wireless Device to Enrol
//1490
Refresh
Close
Sensor ID
Type
Received
Status
Receiver
Signal

//1500
Wireless
ID
All zones have been assigned already!....
Enrol Sensor
Wireless Sensor Enrolment
Wireless Sensor Details....
Sensor ID
Description
Sensor Type
//1510
Zone Type
Add
Cancel
N.B. To Enrol this Wireless Sensor at the panel you must
download the config file to the panel.
Test
Sending SMS Test Command....


//1520
Chime
Autoarm
Area Configuration
Add Area
List
Area
Edit
You have already assigned the maximum number of areas for this panel....

//1530
Yes
No
Configuration details for area....
Chime
Partset Modifiers
Partset A
Partset B
Partset Timed
Partset Access
//1540
Partset Entry/Exit
Partset Local
Delete
OK
Cancel
You cannot de-activate Area 1...
Area 1 must be active at all times...
Delete this area?

//1550
General - Panel Status

N.B. The information below shows the online status information of the panel
(only available when connected to the panel...)
Summary
System
Ethernet
Power
Modem1
//1560
X-BUS
Modem2
Installation Name
Installation ID
IP Address
Installer Name
Installer Phone
Installation Date
Areas
//1570
Users
Zones
Expanders
Firmware Version
Panel S/N
Restore All Alerts
Refresh
Full Engineer
Modem 1 Log
//1580
Modem 2 Log
System Time
Cabinet Tamper
Aux. Tamper 1
Aux. Tamper 2
Bell Tamper
Wireless Module
Antenna Tamper
MAC Address
//1590
IP Address
Netmask
Gateway
Receive
Transmit
Mains
Battery
Battery Voltage
Aux.Voltage
//1600
Aux.Current
Aux Fuse
Ext. Bell Fuse
Int. Bell Fuse
Modem Status
Type Fitted
Line Status
Incoming Calls
Incoming Call duration
//1610
Outgoing Calls
Outgoing Call duration
Failed Dial attempts
Cable Status
Expanders Online
Communication
Cabinet Tamper
Antenna Tamper
RF Interference
//1620
Fuse
Mains
Battery
Offline
Summary
Zones
Areas
System Alerts
X-BUS
//1630
Zone Summary
Refresh Zones
Log
Restore Alarms
Inhibit
Isolate
Soak
X-BUS Summary
Refresh
//1640
System Alerts Summary
Refresh
Restore Alerts
Inhibit
Isolate
Restore
Areas Summary
Refresh
Unset
//1650
Partset A
Partset B
Full Set
Alert
Input
Status
Area
Description
Mode
//1660
ExpanderID
Description
Cable Map
Type
Firmware
Comms
Status


//1670
Zone
Description
Area
Zone Type
Input
Status
Online
Offline
Panel Status Information
//1680
Sending Inhibit command... 
Sending Deinhibit command... 
Sending Isolate command...
Sending Deisolate command...
Sending Zone
Isolate command...
Deisolate command...
Inhibit command...
Deinhibit command...
//1690
Soak command...
Desoak command...
Activating Soft Engineer Mode... 
Activating Full Engineer Mode... 
Requesting zone
log
Quick Log - Zone
Clearing all zone alarms... 
Requesting event log for Modem
//1700
Quick Log - Modem
Clearing all alerts... 
Clearing system alerts... 
Sending Area
Full Set command... 
Controller - Chan.1
Controller - Chan.2
Expander ID

//1710
Cable Fault
Between
and
Panel Configuration Data Printout
Panel Configuration summary printout...
NOTE : This printout extracts information from 
the configuration file stored by SPC Pro.
Refresh Config Data Info
Print
//1720
Cancel
Collating configuration data....
Sending data to printer....
Limited
Standard
Manager
Isolate
Delay Autoarm

//1730
Installation Details
System Options
Timer Values
Users Configuration
Number of users
Area Configuration
Number of Areas
Zone Configuration
Number of zones
//1740
Zone
Area
User
Expander Configuration
Number of Expanders
ID
Wireless Devices
Number of wireless devices
Device
//1750
Installation Name
Installation ID
Panel Type
IP Address
Phone 1
Phone 2
Type
Region
Grade
//1760
Duress
Bell on First
Bell Retrigger
Bell on Fail to Set
Strobe on Fail to Set
Keyfob Restore
PIN Digits
Always Show State
Auto Restore
//1770
Allow Engineer
Allow Manufacturer
Int. Bells
Ext. Bells
Ext.Bell Delay
Ext.Bell Strobe
Chime
Confirm Time
Double Knock
//1780
Soak
Mains Delay
Dialler Delay
RKD Timeout
Wireless Fail to Set
Wireless Lost
Engineer Access
Bell on Fullset
Strobe on Fullset
//1790
Exit Time
Entry Time
Final Exit
Autoarm Warning
Name
Type
Options
Areas
Description
//1800
Expander
Type
Area
Attributes
Description
Serial #
Type


//1810
Sensor ID
Sensor Type
Zone ID
Domestic
Commercial
UK PD6662 compliance
Irish Standards compliance
European Standards compliance
Canadian ULC compliance
//1820
U.S. UL compliance
Engineer
Grade 2
Grade 3
Enabled
Disabled
Minutes
Seconds
Days
//1830
Input
Output
Communications - Serial Port
Settings





//1840
Communications - Modem Configuration
Modem Settings
Modem 1 Primary
Modem 2 Secondary
Enabled

Phone # prefix


//1850
0 to 999 Seconds
Enabled
Modem Type
Country
Answer Mode
Number of Rings
Prefix
Line Monitoring
Line Monitoring Timer
//1860
SMS Enable
SMS Server Number
SIM PIN
Test SMS
(PSTN Only)
(GSM Only)
Test
RedCare Modem Type
Redcare Output Mapping
//1870
Ch1
Ch2
Ch3
Ch4
Ch5
Ch6
Ch7
Ch8

//1880
Never answer Phone
Answer after 'x' RINGS
Ring/Hangup/Ring Sequence
Ireland
UK
Spain
France
Germany
Italy
//1890
India
USA
Canada
Singapore
Finland


Disabled
Alarm
//1900
Confirmed Alarm
Panic
Holdup
Fire
Tamper
Fault
Medical
Arming

//1910
Disabled
Enabled
Fullset
PSTN
GSM
REDCARE
Classic
GSM
Settings
//1920
SMS Test
SMS Message Receiver
Number
Message
OK
Cancel



//1930
Please enter a number to send message to...
SMS Test Successful!
SMS Server Numbers

List of known SMS servers....
Message Server Numbers
N.B. Caller ID must be enabled
Close

//1940
Country / Company
Outgoing Number
Registration
Communications - Alarm Reporting Centres
Add
List



//1950
SIA
Contact ID
Fast Format
SIA Extended 1
SIA Extended 2
Primary
Backup


//1960
Disabled
Hour
Hours
Days
Alarm Receiving Centre
Add/Edit ARC
Add/Edit Alarm Receiving Centre details....
Description
Account
//1970
Protocol
Priority
Number 1
Number 2
Dial Attempts
Test Calls
Identification of Alarm Receiving Centre
Account Number
Protocol used in communication
//1980
Priority of ARC
Phone Number 1
Phone Number 2
Number of dial attempts to connect to receiver
Interval between automatic test calls
ARC Modem Test Call
NOTE: ARC must be programmed on the panel for this test call to be successful....
Filters
OK
//1990
Delete
Cancel
Sending ARC Modem Test Command....
ARC Test Successful!
There is already an Alarm Receiving Centre with that Account number!....
You cannot delete this entry as it is not yet saved....
Are you sure you wish to delete this Alarm Receiving Centre?


//2000
ARC Filters....
ARC Filters
Configure Alarm Reporting Centre settings....
Event Filter
Alarms
Confirmed Alarms
Faults
Arming
Inhibits
//2010
Others
Alarm activation and restores
Alarms confirmed by multiple zones
Fault and Tamper activations
Arming and Disarming
Inhibit and Isolate
All other types of events
Areas
Fast Format Channel Filter
//2020
Channel
Scope
system
OK
Cancel




//2030
Enable
Check this to enable EDP
UDP Port
UDP Port for receiving IP packets (Default is 50000)
Remote Configuration
Check to enable remote configuration of EDP
Remote Password
Password used for remote configuration
Configured Receivers
//2040
Add New Receiver
ID
Description
IP Address
Phone 1
Phone 2
Communications - Enhanced Data Protocol
List
Settings
//2050
Please enter a Receiver ID before saving....
You already have a Receiver entry with this Receiver ID!...
Edit EDP Receiver
Edit Receiver
Edit EDP receiver settings....
Description
Receiver ID
Network Address
Phone Number 1
//2060
Phone Number 2
Description of receiver.
Numeric identification used by EDP to uniquely identify receiver.
Network IP address of receiver.
Dial-up phone number of receiver.
Dial-up phone number of receiver.
Advanced
OK
Delete
//2070
Cancel
Are you sure you want to delete Receiver ID
EDP Receiver - Advanced Settings
Advanced Receiver Settings
Configure EDP settings - Advanced
Security
Network
Dial-Up
Events
//2080
Filter
OK
Cancel
Commands Enable
Encryption Enabled
Encryption Key
Check if incoming commands are allowed from this receiver.
Check if data to and from this receiver is encrypted.
32 Hexadecimal Digits
//2090
Network Enable
Network Address
Network Port
Polling Enabled
Polling Interval
Polling Trigger
Check if events can be reported through Network
Network IP address of receiver. (Leave blank only dial-up)
Network UDP port of receiver.
//2100
Check this to enable IP polling from this receiver
Seconds between polls
Number of missing polls before network fail is registered
Dial-up enable
Dial-up on net fault
Dial-up interval 1
Dial-up interval 2
Check if events can be reported through dial-up
Check if network faults is to generate a dial-up test call
//2110
Minutes between dial-up test calls when network link is up
Minutes between dial-up test calls when network link is down
Primary Receiver
Requeue Events
Event Filter
Check if primary, clear for backup
Check if events that fails to report are to be requeued.
Configure which events are reported to this receiver

//2120
Receiver Event Filter
Event Filter
Configure EDP Event Filter settings....
Alarms
Confirmed Alarms
Faults
Arming
Inhibits
Others
//2130
Alarm activation and restores
Receiver Event Filter
Fault and Tamper activations
Arming and Disarming
Inhibit and Isolate
All other types of events
Areas
OK
Cancel
//2140
Communications - Network Settings
SSL Enabled
Check this to enable encrypted web server
SNMP Enabled
SNMP Community
Check this to enable Simple Network Management Protocol
Community id for SNMP protocol
Portal Registration
Enabled
//2150
Portal IP Address
Portal Port
WAN IP Address
WAN Port
Update Interval
Registration ID:
Last Registration:
Check this to enable portal registration
IP address of portal service
//2160
Port portal server is listening on
IP address of SPC from external network
Port address of SPC from external network
Registration interval in minutes
Ethernet
Portal
Services


//2170
Holidays
Panel Settings - Holidays
Holiday Setup
Holiday valid for this year
Holiday valid every year (Press and hold the 'shift' key when selecting)
Holiday valid for future or previous year
(Press and hold the 'ctrl' key when selecting)
[Tip: Hover the mouse over the holiday to view the holiday # and date...]
Calendar View
//2180
List View
Any
Every Year
Holiday
You have reached the max number of holidays that can be assigned
Holiday Assignment
Select a year for this Holiday
Assign

//2190
Holiday ID
Active
Day
Month
Year
Auto Arming
Configure System Auto Arming
Configure Auto Arming for the System....
Auto Unset
//2200
Auto Set
Sunday
Monday
Tuesday
Wednesday
Thursday
Friday
Saturday
Holiday
//2210
Hr
Min
Quick Setup
Mon-Fri
OK
Save
Enter the Auto Unset/Set times above and click on the 'Update' button
to automatically assign those values Monday-Friday....

//2220
Configure Area
auto arming
Configure Auto Arming for Area
System Timers
Click on the timer value to edit the entry....
Each entry has a maximum and minimum value that must be adhered to......
Identification
Standards
Options
//2230
Timers
Clock
Language
Timer
Value
Units
Min
Max
Description
//2240
Minutes
Seconds
Days
Internal Bells
External Bells
Ext.Bell Delay
Ext.Bell Strobe
Chime
Confirm time
//2250
Double Knock
Soak
Mains Delay
Dialler Delay
RKD Timeout
Wireless fail to Set
Wireless Lost
Engineer Access
Bell on Fullset
//2260
Strobe on Fullset
Exit
Entry
Final Exit
Autoarm Warning
Duration that internal sounders will sound when alarm is activated.
Duration that external sounders will sound when alarm is activated.
Delayed activation of external sounders.
Duration that strobe output will be active when alarm is activated.
//2270
Duration Chime output will activate, when a zone with CHIME attribute opens.
Max time between alarms from two different zones to cause a confirmed alarm.
Max delay between activations of zones with double attribute to cause an alarm.
Number of days a zone stays in soak test before returning to normal operation.
The time that a mains fault need to be present before it is reported.
Dialer delay.
Number of seconds a Keypad will wait for key entry before it leaves the menu.
The number of minutes without supervision that will prevent arming.
The number of minutes without supervision that reports a sensor lost.
//2280
Number of minutes when engineer access will automatically be revoked.
Activate external bell momentarily to indicate Fullset.
Activate external bell strobe momentarily to indicate Fullset.
The number of seconds allowed to leave premises during setting.
The number of seconds allowed to enter premises during unsetting.
Number of seconds to delay arming after final exit is closed.
Number of minutes to display warning before autoarming.


//2290
Set Date/Time
Date
Time
Get PC Date/Time
Send to Panel
Enable
Check to allow SPC Pro to connect to panel.
Engineer Access
Check if engineer access must be granted for SPC Pro to connect.
//2300
Password
Password used by SPC Pro.
Enable IP
Check to allow the SPC Pro application to connect to the system over IP.
IP Port
Select which IP Port SPC Pro will connect on.



//2310
Duress
Bell on Fail to Set
Strobe on Fail to Set
Keyfob Restore
Partset A rename
Partset B rename
Partset Options
Enable CS Message
CS Message Line 1
//2320
CS Message Line 2
Always Show State
Confirmation
If Check this setting if user code +1 should report User duress.
If checked ext. and int. Bell/Strobe outputs activate on unconfirmed alarm.
If checked bells/sirens will resound if a second Zone activation is detected.
If checked then the internal bells will activate when panel fail to set
If checked then the external bell strobe will activate when panel fail to set.
If checked then a second unset triggered through a keyfob will restore alerts.
//2330
Change the Partset A name.
Change the Partset B name.
Change Partset A and B options....
Enable to display a message when panel contacts the Alarm Reporting Centre....
ARC message line 1 (16 chars)
ARC message line 2 (16 chars)
If checked the arming status on the keypad is always displayed.
Sequential Confirmation Mode
Edit
//2340
Installation Date
Panel Settings - System Settings
Domestic
Commercial
Region
Select for compliance to Canadian ULC requirements
Select for compliance to U.S. UL requirements


//2350
Partset Options
Change PartSet A and PartSet B modifiers
Partset A
Partset B
Partset Timed
Partset Access
Partset Entry/Exit
Partset Local
Save
//2360
Cancel
Please enter a value for this timer...
Sending Date/Time.... 
Configure System Alert Policy
Configure Zone Alarm Policy
Configure Zone Tamper Policy
Send Date/Time failed!!...
Function only available when online!....

//2370
Warning!!.... You are disabling
access....
If you download this change to the panel you will not be able
to connect to the panel using
Are you sure?...
You have selected to change to a grade which may affect your timer values.
Any values that are outside the min/max allowed for this grade
will be adjusted automatically.
Do you wish to continue?
//2380
Changing grade - Timers warning....
Your user code digits is currently set to four.
Changing to this grade
will automatically modify your codes to 5 digits
Do you wish to continue?
Changing grade - User code warning....



//2390
Controller Mains Fault
Controller Battery Fault
Controller Aux. Fuse Fault
Controller Ext. Bell Fuse Fault
Controller Int. Bell Fuse Fault
Controller Bell Tamper
Controller Cabinet Tamper
Controller Aux. Tamper 1
Controller Aux. Tamper 2
//2400
Controller Antenna Tamper
Controller RF Jamming
Modem 1 Fault
Modem 1 Line Fault
Modem 2 Fault
Modem 2 Line Fault
X-BUS Cable Fault
Fail to Communicate
User Duress
//2410
Expander Status

Expander Status Details....
Expander ID
Type
S/N
Firmware Version
Voltage
Battery Voltage
//2420
Current
Restore Alerts
Inhibit
Isolate
Close
N/A



//2430
Communication
Cabinet Tamper
Fuse Fault
Mains
Battery
RF Jamming
Antenna Tamper
Panic
Soak
//2440
Isolate
Inhibit
Restore
Deisolate
Deinhibit
Sending Inhibit command... 
Sending Deinhibit command... 
Sending Isolate command... 
Sending Deisolate command... 
//2450
Clearing expander alerts
Please select an alert from the grid above....
Desoak
Configured as Ring Net
Chan.1 - Position
Chan.2 - Position
Sending Area
Partset A Command... 
Partset B Command... 
//2460
Reading Status.... 
Unset Command... 
Unknown Type
bytes
Modem Disabled
Seconds
Input
Output

//2470
Function only available when panel is online....
Please select a zone from the grid above....
Please select an area from the grid...
Panel Settings - Expanders && Keypads
Add New Expander
Re-assign Expander IDs / Serial Nums
Auto-assign serial numbers from Panel Nodes
Settings
List
//2480
<Unassigned>
Maximum number of expanders has been reached!...
Function only available when online with panel...
Maximum number of keypads has been reached!...
Maximum number of I/O Expanders has been reached!...
No expanders yet configured!



//2490
X-BUS Settings
Configure ENET settings....
X-BUS Type
Retries
Timeout
Attempted retransmissions in case of interference.
(Default is 25).
Seconds a connection interference must be present before alert reported
(Default is 10)
//2500
OK
Cancel
Closed Loop
Open Loop
Expanders
Re-Assign Expanders
Select an expander and use the UP/DOWN buttons to reposition...
Use the arrow buttons on the right to re-assign Expander IDs.
To swap serial numbers double-click on an Expander....
//2510
N.B. Any configured zones/outputs will remain with the Expander ID.
Move selected Expander up ID list
Move selected Expander down ID list
Apply changes to Config file now...
Position
Expander
Type
Serial #
Description
//2520
Swap Expander serial number
with
[8In / 2Out]
[8Out]
These expanders will now be reassigned - Continue?
Please select an expander from the grid...
Swapping serial numbers is only allowed between expanders of the same type...
There are no other expanders of this type configured....
Expander Serial Number problem!!!
//2530
Zone
Description
Type
Attributes
Area
Modify EOL for All System Inputs
Inputs
Outputs

//2540
Panel Settings - Controller Inputs && Outputs
Output
Description
Type
Assigned as:
Type
Invert
Log
Test Outputs
//2550
Refresh Output Status
<Assigned>
Continuous
Momentary
Pulsed
<Area Output>
<System Output>
<Zone Mapped>
<Access Door>
//2560
Area
System O/P
Zone
Sending Output
Set OFF command... 
Set ON command... 
Reading Outputs Status.... 


//2570
Edit Input
Configure Input Settings....
Input
End of Line
Analysed
Pulse Count
Gross Attack
Zone
Description
//2580
Type
Area
Attributes
OK
Cancel
Please select valid zone type from list...
Output Edit
Edit Output
Configure Output settings....
//2590
Output Type (Mapping)
System Output
Area Output
Zone Mapping
Description
Mode
On Time
Off Time
Invert
//2600
Log
[100ms]
OK
Cancel
Select a system output function....
Select an Area number and an output function within that area....
Select a zone to map this output to....


//2610
Edit Expander
Configure the settings for this expander
Expander ID
Type
Serial #
Description
Output
Description
Type
//2620
Assigned as:
Mode
Invert
Log
Refresh Output Status
Test Outputs
OK
Delete
Cancel
//2630
Input
End Of Line
Analysed
Pulse Count
Gross Attack
Zone
Description
Type
Attributes
//2640
Area
Keypad Options
Areas assigned to this keypad
Backlight
Indicators
Buzzer
PACE Entry
Panic
On when key is pressed
//2650
Always ON
Always OFF
Enabled Visible Indicators
Enable keypad buzzer
Disable keys during entry time
Using 2 soft keys
Inputs
Outputs

//2660
Disabled
Enabled
Enabled (Silent)
Edit Expander Input
Sending Output
Set OFF command... 
Set ON command... 
Continuous
Momentary
//2670
Pulsed
Reading Outputs Status.... 
System O/P
Zone
Delete Expander ID
Are you sure?
Cancel
<No events found>

//2680
Date/Time
Event
Receiver
Signal
Status
Battery
Type
Number
Result
//2690
Modify System EOL
System End Of Line value
Set EOL value for all inputs (Controller & Expanders)....
Select End Of Line Type
OK
Cancel



//2700
Swap Expander......
Expander Swap
Choose Expander to swap Serial Number with...
Cancel
Swap
ID
Type
Serial #
Description
//2710
Swap serial number
with
Please select an Expander from the list...
This will download the full config file... Are you sure?
Changes to expander configuration will now be made... Continue?
WARNING - Panel is in Full Engineer mode!!
If you disconnect now all alarms on panel will continue to be disabled....
Are you sure? (Y/N)

//2720
Problem Compressing the file - Configuration not sent to panel!!!
File does not exist!!!
Please select a file to Import....
Error decrypting the config file!!!
SPC Pro failed to allocate the serial numbers
there are still some unallocated...
Sending Firmware file to panel....
Importing config file

//2730
Expanders Issue!....
The number of expanders in the config file does not match the number
of expanders on the panel....
expanders on Panel
expanders in Config File
Abort
Expander types Issue!....
The expander types on the panel do not match
the expander types in the config file...
//2740
in Config file
on panel
You cannot send the config file to this panel unless all expander types match
between panel and SPC Pro!...
Keypad
I/O [8In/2Out]
I/O [8Output]
Analysed
PSU
//2750
Wireless
Expanders Issue!....
The number of expanders in the config file does not match the number
of expanders on the panel....
expanders on Panel
expanders in Config File
Abort
Reading X-BUS Expander Info.... 
SPC Firmware
//2760
!!! Problem occurred trying to parse the Panel Log data....
Getting Zone Status.... 
Please wait while files are deleted....
Getting Unenrolled Wireless Devices.... 
Device is not a SPC Fast Programmer....
Connected device is not a SPC 5000 or SPC 6000 panel...
Comms Error - Connection to panel has failed... 
Connected panel type is different from the saved setting for this config file
Panel
//2770
File
Do you wish to change the file setting to match this new panel type?
Wireless - ID
Input
Output
Soft Engineer
Full Engineer


//2780
Inhibit/Deinhibit command failed!
Isolate/Deisolate command failed!
Soak/Desoak command failed!
Change Engineer Mode command failed!
Error occurred performing Zone Log command... 
Clear all zone alarms command failed!
Problem occurred retrieving Modem Log...
Clear all alerts command failed!
Error occurred performing Area Fullset command... 
//2790
Error occurred performing Full Set command... 
Error occurred performing Area Partset A command... 
Error occurred performing Area Partset B command... 
Error occurred performing Partset B command... 
Error occurred performing Area Unset command... 
Error occurred performing Unset command... 
Failed to connect to panel!.... 
X10 Output State Change command failed!
Problem occurred getting file from programmer 
//2800
Problem reading the Device Info details of Fast Programmer
Update Zone Status failed!...
Update Panel Status failed!...
Update Output Status failed!...
Error occurred getting Device Info... 
Getting Unenrolled Wireless devices failed!...
Output State Change command failed!
Error occurred sending file to programmer.... 
Problem occurred while compressing the file!... 
//2810
ARC Test failed!....
Error occurred performing Sensor Log command... 
Problem occurred trying to retrieve log....
Keypress Send failed!...
Sending file to panel failed.... 
Retrieving Datestamp Info failed.... 
Failed to retrieve config file from panel... 
Change Engineer Mode command failed!
Clear expander alerts command failed!
//2820
SMS Test failed!....
Retrieving Datestamp Info failed.... 
Firmware upgrade failed!...
Error decrypting the config file!!!
Free Space
Used Space
Bytes


//2830  '-- Error messages start
OK
Cannot reset after firmware update (lost connection)
Could not dial out
Modem pre-init failed
Modem didn't respond to pre-init string
Modem failed to connect after dialling
Socket connection lost
Socket connection closed
No carrier
Command timeout
Could not allocate memory
Could not decompress
Received wrong decompressed size
Unable to open destination file
Y-modem transfer failed
Invalid arguments
Only allowed in engineer mode
Not allowed in engineer mode
Internal error
Invalid area
Unable to arm because of zones open
Unable to arm because of zones in alarm
Unable to arm because of zones in tamper
Unable to arm because of system alerts
Could not allocate memory
Invalid zone id
Unused zone id
Invalid node id
Invalid alert id
Cannot act on User Duress
X-10 Not enabled on controller
Modem Busy
Modem Fault
Failed to send
Access denied! SPC Pro access disabled in panel
Access denied! engineer access required
Access denied! bad password
Already in engineer mode
Unable to exit engineer mode, faults and tampers must be cleared first!
Not in engineer mode
Invalid sensor id
Phone number too big
Invalid modem number
Modem is not enabled
Unsupported command
Invalid file type (internal error)
File Reception failed
File Transmission failed
Invalid file
Unavailable language
Could not save file in flash
Unknown error type!!!
Group ID is Invalid






//2890  '-- OCX return codes
Ok and Complete
Ok and in progress
Could not open the port/file for reading
Port/file read failed
Could not write the port/file for writing
File is invalid
Error: busy with previous command
Not connected to panel/programmer
Cannot open COM port
Could not send command to controller or fp (bad connection)
Cannot get file size
Bad arguments
Winsock error
Cannot allocate memory
Invalid file type
Invalid file size
Invalid file CRC
Cannot connect as already connected or connecting
Internal error
Carrier lost
Cannot connect over TCP/IP (invalid or unreachable IP address or TCP port)
Modem init string failed
Modem dialling failed
Unknown error type!!!
Not Ready
Command is not implemented...
A timeout occurred
Transfer failed
Connection failed
//2920









//2930
Port 1 in use - X10 Enabled
Port 2 in use - Modem 2 Enabled
English (North America)
French (Canada)





//2940
Keypads
Keypad Summary
Configured Keypads
Expanders
Max number of keypads has been reached!
Delete Keypad ID



//2950
The SPC Pro password has been changed!....
Do you want to modify the SPC Pro installation data file to match?
Panel Version






//2960
Dual 6K8/4K7
Dual 4K7/4K7
Dual 3K0/3K0
Dual 3K3/3K3
Dual 5K6/5K6
Dual 2K7/8K2
Dual 3K9/8K2
Dual 1K0/470

//2970
Version
The SPC Pro config file is not compatible with the
firmware version of the connected panel!!
Panel Version
Config File
SPC Pro will now disconnect....
Upgrade
You already have an installation with that ID
please change the Installation ID
//2980
Upgrade Firmware Version
Upgrade to Version 1.3
Upgrading Firmware Version to 
Upgrade to
complete!...
Firmware Ver.
This Firmware Upgrade function will modify the SPC Pro
config file for this installation entry....
It cannot be undone - Are you sure you wish to continue?
//2990
N/A
Ready
Detecting
Initializing
Dialing
Answering
Connected
Disconnecting
Busy
//3000
Unknown
Disabled
Ok
No Response
Fault
Bad Pin
Line Fault


//3010
PSTN
GSM
Redcare
OK
Alert
Inhibit
Isolate
Fault

//3020
Unset
PartSet A
PartSet B
Full Set
Unknown
Closed
Open
Short
Disconnect
//3030
Masked
DC Sub
Sensor Missing
Unknown





//3040        
OK
Inhibit
Isolate
Soak
Tamper
Alarm
Unknown


//3050
Online
Offline
Lost
Pending
Check to enable engineer to control panel through SMS
SMS Events
SMS Control
Show Open Zones
If checked then open zones will be displayed on keypad in Unset mode.
//3060
Close
Tamper
Open
Controller
Expander
High
Low


//3070
Keypad Status
Keypad Status Details....
Keypad ID
Please enter a valid group name!....
Group name already exists....




//3080
English (N.America)
French (Canada)
Swedish
Norwegian
Danish
Czech
Polish


//3090
Tech Zones Report
Tech Zones Display
Tech Zones Audible
Tech Zones Delay
Tech. Delay
Number of seconds to delay triggering of tech. zones 
with tech. delay attribute.


//3100
Advanced
Calendars
Triggers
Mapping Gates
X-10
License
Week Type


//3110
View/Edit Selected Trigger
Create New Trigger
Add New ON Trigger
Add New OFF Trigger
Positive
Negative
ID
Trigger Description
<No Triggers Configured>
//3120
Please select a trigger from the grid...
Loading Trigger Data....
Please select a trigger from the grid....
The Maximum number of triggers has been reached!
Loading Trigger Data....
Select Trigger
Edge
Assign
Cancel
//3130
Create New Trigger
View Selected Trigger
Mapping Gate Triggers
Configure ON/OFF triggers for Mapping Gates....
Trigger ON
Trigger OFF
Remove Trigger
Add ON Trigger
Add OFF Trigger
//3140
Close
Please select a trigger from the grid...
ID
Trigger
Edge
Advanced Settings - Mapping Gates
Mapping Gate List
Output
Keypad
//3150
Triggers
<NONE>
Trigger(s) assigned
Loading Mapping Gate Trigger Data....
Advanced Settings - Triggers
Triggers List
Triggers Listing
Add New Trigger
ID
//3160
Description
Number of Trigger Conditions
Configure Generic Public Holiday
Trigger Conditions
Loading Trigger Data....




//3170
Trigger Configuration
Configured Conditions for this Trigger
Trigger Num
Trigger Description
Active Time
Time Limitation
to
Calendar
View Selected Calendar Settings
//3180
Create New Calendar
Trigger Conditions
Zone
System Output
Area Output
Wireless FOB
Keypad Code
Time Condition
Calendar
//3190
Delete This Trigger
Remove Selected Condition
Cancel
OK
<No Calendar>
ID
Input/Output Conditions
SYSTEM OUTPUT
AREA OUTPUT
//3200
ON
OFF
Area
Zone
OPEN
CLOSED
DISCONNECT
SHORT
Before Time
//3210
After Time
Equal to
KeyFOB
Any User
User
Keypad Code
Trigger Condition
Configured Conditions for this trigger....
System Output
//3220
State
Cancel
Assign to Trigger
Zone Condition
System Output
Wireless FOB
Keypad Valid Code
Time Condition
Calendar
//3230
System Output Condition
Wireless FOB Condition
Keypad Code Condition
Time Condition
Calendar Condition
Area Output Condition
Select Zone and Zone state....
Select Output and Output state....
Select individual FOB or ANY FOBs....
//3240
Select individual Code or ANY code....
Select time condition....
Select Calendar (uses active times)....
Select Area, Output and Output state....
<No Calendars Configured>
Number of seconds trigger conditions must be true.
Zone
Zone Condition
Keypad Valid Code
//3250
Area
Area Output
Output State
Delete this trigger - This will delete the trigger and all it's conditions!...
Continue?
Delete Warning
Remove the condition
Please select a trigger condition to remove...

//3260
ON Time
OFF Time
On/Off Time
Remove selected trigger from list?...
Continue
Remove
Addressing Mode
Manual
Automatic
//3270
Retrigger
Select a Mapping Gate to map this output to....
Output Mapping
Output Configuration
Calendar
Disabled
Automatic
Supervised
Fullset
//3280
Unset
Automatic Area Setting/Unsetting
Configure Auto Set/Unset for Area
Automated SMS #
Automated SMS Interval
Incoming Calls
Only answer when engineer access is granted


//3290
Disabled
1 Hour
24 Hours
48 Hours
7 Days
30 Days



//3300
Protocol Version
Select version of EDP protocol to use with this receiver
Version 1
Version 2
Test All
Check if all modems should be tested
Maximum number of calendars has been reached!...
<Mapping Gate>

//3310
Swedish
Norwegian
Danish
Czech
Polish




//3320
PACE + PIN
Restore on Unset
Offline Tamper
If checked then both a PIN code and a PACE is required.
If checked then alerts will auto clear 30 secs after Unset.
If checked then expander zones that goes offline will generate a zone tamper.
Duress
Report user duress if 'code + 1' or 'code + 2' is entered on keypad
Disabled
//3330
Code + 1
Code + 2
Tech.Delay
Number of seconds to delay triggering of tech.zones with tech.delay attribute.
Check to enable user to receive SMS events
Tech Zones Report
Tech Zones Display
Tech Zones Audible
Tech Zones Delay
//3340
Loading Calendar Data....
ID
Description
Start Date
End Date
Maximum number of exception days has been reached!...
Public Holiday
Clear this Exception Day?
Assign this Exception Day?
//3350
Week
Layout
From
to
ON Time
OFF Time
Week Type


//3360
Date/Time Scheduler
Assign Week Types to week numbers
Week Numbers :
Calendar :
Description :
Select Year :
Week Types :
Assigned Exception Days :
View/Define Week Types
//3370
Unassign Selected Day
Add/Edit Exception Days
Assign selected week type to all week numbers
Clear week types from all week numbers
Assign all weeks as Week Type
Refreshing Calendar Data....
Clear all week type assignments?
Updating Calendar......

//3380
New Exception Day
Create New Exception Day...
Assign as generic Public Holiday
View/Edit Exception Day
Existing Exception Days
Clear Exception Day
Week Data
Show On/Off schedule for this Week
Delete this calendar - Are you sure?
//3390
Groups Filter :
Cause & Effect
<Not Assigned>
SMS Authentication
Authentication of received SMS control commands. 
Pin Code Only
Caller ID Only
Pin and Caller ID
SMS Pin code only
SMS Pin and Caller ID
Keypads Issue!....
The number of keypads in the config file does not match the number
of keypads on the panel....
keypads on Panel
keypads in Config File
Abort



//3410
The file you have selected is not a SPC Pro Configuration file....
Copy Firmware to Programmer
Copy Now...
Fast Programmer window was closed...
No Keypads yet configured!
Auto Status Refresh
Not Fitted
Type
View PSU Status
//3420
Link Missing
12V Mode
7AH Battery
17AH Battery
--
If checked then signals received with low signal strength will be disregarded.
Filter


//3430
RF Type
RF Version
Date && Time
Automatic Daylight Saving Time
Synchronize time with Mains
User Duress
Technical
Zones Omitted

//3440
Changing to Manual Addressing Mode will result in an automatic 
Expander reconfiguration
Some zones may be moved during this process....
You cannot configure panel for Manual X-BUS as there are non-addressable Expander 
type(s) already configured...
Expander ID is already in use!
Show All Zones


//3450
Position
ID
Status
Type
S/N
Description
Online X-BUS Map Summary
List of Expanders/Keypads physically connected to the panel....
Refresh
//3460
Ring
Multidrop
Close
Topology
Port
Expander types are configured which do not support manual addressing...
X-BUS will remain configured as Automatic
You cannot assign the panel for Manual X-BUS addressing as there are 
non-addressable expanders connected to it!
//3470
Click OK to change config file assignment to Automatic X-BUS addressing
before downloading?
N.B. : When X-BUS addressing set to 'Manual', Expanders with an ID value 
greater than 63 will not have ANY zones assigned!...
IMPORTANT! - Configuration update....
The application has detected that your config files may have been generated
by an earlier version of SPC Pro.
Your configuration files will be updated now....
OK
//3480
Checking and updating configuration files... Please wait....








//3490









//3500
SPC4000
SPC5000
SPC6000






//3510
Keypad Configuration
Number of keypads
ARC ID does not exist on panel...
You have at least 1 unconfigured Expander/Keypad connected to the panel!!
No Areas configured on panel....
SMS Setup
SMS Events
SMS Control
View/Edit SMS Events
//3520
View/Edit SMS Control
SMS Event Reporting for User
You must save this user before you can create/modify SMS options....
SMS Control for User
SMS Event Reporting
Configuration details for SMS Event Reporting.....
Enable
Number
Alarm Activation
//3530
Confirmed Alarms
Fault & Tamper
Arming & Disarming
Inhibit & Isolate
All Other
(In order to delete an entry, leave number blank)
Save
Cancel

//3540
Enable
Number
PIN
Commands Enabled for this User
Check to enable SMS Messaging
Caller ID of User's Phone
Authentication PIN
Command
Description
//3550
Allows Full Set of alarm by SMS
Allows Unset of alarm by SMS
Allows access to Status
Allows access to Event Log
Allows controlling access to Engineer
Allows controlling access to Manufacturer
Allows control of outputs
Allows control of X10 outputs
OK
//3560
Cancel
Number of seconds to display fail to set message (0 = until valid code entered)
Installation Type
View X-BUS Map
Add New Keypad
Detect RF Jam
If checked then an alert is activated if RF interference is detected.
ARC Log

//3570
Configured Cause && Effect List
Cause/Effect List
Cause && Effect Listing
ID
Type
Item
Description
No. of Triggers
Add New Cause/Effect
//3580
Cause && Effect Configuration Wizard
Create and configure Cause && Effect objects....
Step
of
Select Item you want to Trigger :
Select the type of item that you wish to trigger.
Can be either an X10 device or Mapping Gate.
Click the 'Next' button to begin configuring this device and the conditions
that will trigger it.
//3590
Next
Close
Select device type to trigger
<Select Item>
X-10 Device
Output Control
NONE
Enter Description for Mapping Gate :
Key # for this output (optional) :
Assign a description to the Mapping Gate and a keypad key that will toggle
this output (if required)....
Add ON Trigger
Remove Trigger
Add OFF Trigger
Add/Remove triggers to turn ON or turn OFF your selected device....
Each trigger has a number of conditions that when met will trigger the device.
Click on a trigger to see the conditions that make up that trigger.
Trigger ON
Trigger OFF
//3610
Select Mapping Gate Number :
Select a Mapping Gate from the list. This is the device that will be triggered.
Expander Output Assignment :
Add New Assignment
The Mapping Gate MUST be mapped to an output on one of the connected expanders.
When the Mapping Gate is switched the mapped Expander output(s) will trigger.
You can assign/map the Mapping Gate to more than 1 Expander Output....
Enter Description for X10 Device :
Key # for X10 Device (optional) :
//3620
Select the X10 device, Description and Keypad Key number (if required)....
Select X10 Device :
Select the X10 device
Cause & Effect can only be configured for X-10 and Mapping Gates!...
Please select a Device type from the list....
Configure X10 Description/Keypad
Assign/Create Triggers
Select Mapping Gate Number
Enter Mapping Gate Description & Keypad Key #
//3630
Assign Mapping Gate to Expander Output
Assign/Create Triggers for switching the Mapping Gate
Please Select a Mapping Gate number from the list!...
Mapping Gate
Expander ID
Serial #
Expander Description
Expander Output
Controller
//3640
Controller/Expanders - Outputs && Assignments :
Assign selected output as Mapping Gate
Clear Selected Output
Close
Assign selected output as Mapping Gate
Change output type from
Clear output type?
Modify Expander
Output
//3650
System Output
Area
Zone Output - Zone #
Door Output - Door #
Mapping Gate
Unknown!!!
Expander ID
SN:
Controller
//3660
Modify Controller - Output
Finish
Back
Configured Calendar List
Calendar List
Calendar Listing
ID
Description
Week Type Assigned
//3670
Add New Calendar
Configure Generic Public Holiday
View/Configure Exception Days
Exception Days
These time entries will override the normal week type times assigned
to the respective calendar....
Add New Exception Day
Remove Unused Exceptions
Remove Expired Exceptions
//3680
Close
ID
Description
Start Date
End Date
In Use
ON
OFF
This will delete all exception day entries that are not assigned to a calendar... 
//3690
Continue?
Maximum number of exception days has been reached!...
This will delete all exception day entries that have expired... 
Continue?
Exception Day Config
Each day has 4 ON and 4 OFF times....
Description
From Date
To
//3700
On Time
Off Time
Calendars Assigned to
Auto Assign to All
Delete
Cancel
Save
Exception Day
Are you sure you want to remove this Exception Day?
//3710
Each Day has 4 ON/UNSET and 4 OFF/SET times....
On/Unset
Off/Set
NOTE: Uncheck the timebox to disable that time.
A single ON or OFF time is considered to be an instant trigger time....
Save
Modify Day parameters....
Generic Public Holiday - On/Off times....

//3720
Show items Calendar is assigned to....
Delete this Calendar
OK
Week Types Configuration
Define Week Type days/times settings....
Type 1 Description :
Type 2 Description :
Type 3 Description :
Day Of Week
//3730
ON/Unset
OFF/Set
Show Week View....
Close
Copy On/Off Times
Paste On/Off Times
Clear On/Off Times
Week Type
Enable
//3740
Scheduler Week Layout
Grid below shows On/Off times for selected week.....
Day
AM
PM
Close
N.B. This trigger will only become active when ALL of the conditions below are
met at the same point in time.
If you assign a 'Time Limitation' or 'Calendar' to this trigger then this will
//3750
further limit the trigger to be active only when ALL condition are met
AND within a valid time On/Off duration.
ON
OFF
Assign Now
Not Assigned!!!
Mapping Gate #
Mapped to
Keypad Quick Key
//3760
Show Expander Assignment
N.B. When ANY one trigger in this list has ALL of it's conditions met then the
Mapping Gate will be triggered ON...
Mapping Gate will be triggered OFF...
Clear
OK
Sending Command to turn Mapping Gate
OFF...
ON...
//3770
Mapping Gate State change failed!...
Clear Mapping Gate?
N.B. When ANY one trigger in this list has ALL of it's conditions met then
then X10 device will be triggered ON...
then X10 device will be triggered OFF...
!!! FILTER IS ON !!!
Filter Zones :
All Zones
Calendar not assigned to any items....
//3780
Controller Output
Expander
Keypad
Zone
Area
User
Trigger
ID
Output
//3790
Calendar Assignment...
Warning : This calendar is currently assigned to the above items!....
Cancel
Delete Calendar
CURRENTLY ASSIGNED TO..
Lower version panel - Command not supported
Parsing error
Panel Signature Mismatch Upload

//3800
Engineer Reset
Require engineer restore of zones after confirmed alarm.
Please enter a user code...

Sweden
Norway
Denmark
Czech
Poland
Russia
Slovakia
Slovenia
Netherlands
Lithuania
Turkey
Romania
Latvia
Portugal
Switzerland
//3820
Command not supported
Frame parse error
Serial Enabled
USB Trace Enabled
Access Denied
Access Denied - Engineer
Access Denied - Password
Invalid Command
Transfer Complete
//3830
Transfer Failed
Invalid Command File
Active
Licensed
Unlicensed
Language Option not available on panel
The Maximum number of triggers has been reached!
Loading Trigger Data....

//3840
For further information please refer to the SPC Pro Configuration Manual
General - Panel Access Log
Panel Access Log
Any User
Any Door
Door
Access Log
User
Door
//3850
Get Current Date & Time
Get Access Log
Time
User
Door
Event
Save Log to File
Access
Requesting Access Log File....
//3860
Remote Maintenance Report(s)
Maintenance Report
Maintenance Filter






//3870
All Panels
Not Configured for Maintenance Reports
Last Maintenance Report Passed
Last Maintenance Report Failed
Maintenance Report Overdue
Awaiting First Report
New Report - Not yet reviewed...


//3880
Last Service Passed
Issue(s) Found in Report
Service Overdue
Awaiting First Report
New - Review required...




//3890
Copy/Create New Installation
Remote Maintenance Reporting
Get Maintenance Report for this Installation
View Saved Maintenance Reports for this Installation
Copy Area Settings
Paste Area Settings
Copy Zone Settings
Paste Zone Settings
Copy Calendar Settings
//3900
Paste Calendar Settings
Copy Calendar Settings
Paste Calendar Settings
Copy Output Settings
Paste Output Settings
Enter details for this installation....
Maintenance Report Schedule
OK
Modify the details to be saved for this installation....
//3910
Remote Maintenance Report Schedule
Enable
Next Scheduled Report Date
Frequency
OK
Cancel
Months


//3920
Maintenance Report Options
Request Maintenance Report
View Archived Maintenance Reports
Close
Maintenance Reports for installation ID
View Selected Report
Close
Report Date
Report ID
//3930
Status
Loading Report....
There are no archived maintenance reports stored for the selected installation...
Maintenance Report request for Installation
has been queued
Copy Firmware File to Programmer
New Remote Maintenance Status Update
Installation

//3940
Remote Maintenance Setup
Remote Maintenance Report Configuration
Enable
Installation ID
Password
Report Path
Next Expected Report Date
Server Primary IP Address
Server Primary IP Port
//3950
Server Backup IP Address
Server Backup IP Port
Server Primary Modem #
Server Backup Modem #
Enable Remote Maintenance
Unique Remote Maintenance ID (1 to 999999)
Remote Maintenance password to use
Report Schedule path
Date/Time when panel should send next report..
//3960
IP address or DNS of primary server
IP Port of primary server
IP address or DNS of backup server
IP Port of backup server
Modem number of Server's Primary Modem
Modem number of Server's Backup Modem
Service Setup
Not Scheduled
Send by IP
//3970
Send by Modem
All Doors
Configure Doors on the panel.
Remote Service Report for Installation ID
Panel Remote Service summary report....
NOTE : This is the summarised Remote Service Report....
Show Full Service Report
Save As...
Print
//3980
Close
Reloading Report... please wait....
Show Short Service Report
NOTE : This is the Full Remote Service Report....
Show Full Service Report
NOTE : This is the summarized Remote Service Report....
Save Remote Service Report as file...


//3990
REMOTE SERVICE REPORT - Date
INSTALLATION
ADDRESS
INST. ID
SYSTEM INTEGRITY CHECKS
TIME AT PANEL BEFORE CALL :
SYSTEM LAST SET
SYSTEM LAST UNSET
LAST ALARM IN AREA(S)
//4000
COMMUNICATIONS TESTED AND OPERATIONAL
ZONE/DETECTOR CHECKS
DETECTORS SOAKED TEST
DETECTORS INHIBITED/DISABLED TEST
DETECTORS REPORTING VALID STATES
SYSTEM ELECTRICAL CHECKS
MAINS SUPPLY HEALTH
CONTROL PANEL BATTERY
PANEL FUSE(S) CHECK
//4010
PANEL TAMPER(S) CHECK
X-BUS CABLE CHECK
X-BUS DEVICES CHECK
X-BUS NETWORK CHECK
EXPANDERS STATUS/TAMPER CHECK
KEYPADS STATUS/TAMPER CHECK
PANEL LOG EVENTS


//4020
Door Controllers
Doors
Door
DPS
DRS
Door Mode
Lock
Unlock
Normal
//4030
Momentary
Refresh Doors
Door Controller Status
Controller Status
Door Controller status details....
Getting Door Status....
Update Door Status failed!...


//4040
Closed
Open
Short
Disconnect
N/A
DC Substitution
Offline


//4050
OK
Open Too Long
Left Open
Forced Open
Tamper
Offline
Normal
Locked
Unlocked
//4060
Sending command to Lock Door
Sending command to UnLock Door
Sending command to Return Door to Normal
momentarily....
Door configuration
Configure the I/O settings for this door....
Door Inputs
Door Attributes
Door Timers
//4070
Door Calendars
Door Triggers
Zone
Description
Zone Type
Zone Attributes
Area
Door Position EOL
DPS Normal Open
//4080
Door Release EOL
DRS Normal Open
Door Group
Card and PIN
PIN only
PIN to exit
PIN to unset
Emergency
Escort
//4090
Prevent Passback
Soft Passback
Custodian
Sounder
Ignore Forced
Door Locked
Door Unlocked
Edit Door Triggers
OK
//4100
Cancel
Not Grouped
Door Group
Parameter
Value
Description
Units
Min
Max
//4110
Zone
Select Zone allocation
Description
Enter door/zone description.
Zone type
Select zone type
Zone attributes
Click to edit zone attributes.
Door Position
//4120
Select End of Line resistor configuration for door position input.
DPS Normal Open
Check if door position input sensor is Normal Open
Door Release
Select End of Line resistor configuration for door release input
DRS Normal Open
Check if door release input sensor is Normal Open


//4130
Access granted
Time the lock will remain open after granting access
Access denied
Time controller will wait after invalid event
Door open
'Door Open too long' alarm if door is open longer than this time
Door left open
'Door Left Open' alarm if door is open longer than this time
Extended
//4140
Additional time after granting access to a card with 'Ext. time' attribute
Escort
Duration to grant escorted access after a card with 'Escort'
Seconds
Minutes
None
View Selected Calendar Settings
Create New Calendar
Edit
//4150
You have not yet selected a zone number to edit...
Loading Calendar Data....
Please select a Calendar...
Door Controller
Input
Zone Attributes for Zone
Edit the zone attributes
OK
Cancel
//4160
Door Triggers
Add triggers for Lock, Unlock and Normal door operation....
Triggers that will Lock Door
Triggers that will Unlock Door
Triggers that will Set Door to Normal
Add Trigger
Remove Trigger
Close

//4170
Door Normal Trigger
Door Lock Trigger
Door Unlock Trigger
Door
Location
Zone
Group
Area
Panel Settings - Doors
//4180
Door Controller
I/O
Door Group
Door List
Input
Door Controller Summary
Door Summary
Door Controllers

//4190
Configured Door Controllers
Expander
Type
Serial #
Description
Inputs
Outputs
Add New Door Controller

//4200
Door Options
Door I/O
Edit
Door assignment has changed... 
You need to save these changes before you can modify the door data. 
Save now?....
You cannot assign the same door number to both door inputs!!.....
Input
Output
//4210
Zones/Outputs
Door Configuration
Configure the I/O settings for this door....
Door Input 1 (DPS) : 
Zone :
Description :
Zone Type :
Zone Attributes :
Area :
//4220
EOL :
Edit
Door Output : 
Description :
Configure Output
OK
Cancel
Door Input 2 (DRS) : 

//4230
You have not yet selected a zone number to edit...
User Output
Door Output
ZONE OUTPUT
DOOR OUTPUT
USER OUTPUT
Door Number
Calendar Assignment

//4240
Door ID
Location
Zone
Group
Area
Entry Granted
Entry Denied
Exit Granted
Exit Denied
//4250
Door Open Too Long
Door Left Open
Door Forced
Door Normal
Door Locked
Door Unlocked
Fail to Communicate
Door Lock
Door Unlock
//4260
User Card
Door Control
Door ID is invalid (too big)
Door with given Door ID is unused
Invalid user ID
Inactive user ID
Cannot act on User Panic
Cannot act on User MDT Alarm
Doors
//4270
Door Events
User
User Name
Door
Door Description
Event
Door Condition
Select Door number and Door state....
Engineer Lock
//4280
Engineer Lock PIN
If checked the Engineer lock PIN code is required to factory default the panel
Four digit engineer lock code.
RF FOB Panic
Select how the Panic buttons on the RF Fob should operate.
Disabled
Enabled
Enabled (Silent)
Armed Report Only
//4290
Select the calendar to use for auto set/unset times.
You can enable or disable Fullset and Unset functions - 
when set to 'Supervised' a signal will be sent to Central Station 
if the location fails to set/unset...
Automatic Setting/Unsetting
Configure Auto Arming for the System....
Duress
Tech
Zone Omit
//4300
GPRS Settings
External Modem
CDMA Relay Reset
Enabled
GPRS Settings for modem
GPRS Acess Point Name
GPRS User
GPRS Password
OK
//4310
Cancel
DNS Server
You have just copied from this device - Cannot paste!...
Paste settings from Area
to Area
Continue?
Paste Area Settings
Paste settings from Calendar
to Calendar
//4320
Continue?
Paste Calendar Settings
Paste settings from Zone
to Zone
Paste Zone Settings
Paste settings from Output
to Output
Paste Output Settings

//4330
User Output
Output
Unit
Assigned to following Controller/Expander Output(s)
Add new Controller/Expander output assignment
OK
Access Control
Add/Edit Access Control Card
You must save this user before you can modify Access options....
//4340
Access Control Config. for User
Card/Door Details....
Card Details
Card Attributes
Door Assignment
Card Format
Card Number
Site Code
Select format of access card
//4350
Enter card number
Enter site code. (Wiegand and HID card formats only)
Extended time
Unset outside
Unset inside
Fullset outside
Fullset inside
PIN bypass
Priority
//4360
Escort
Custodian
Check to extend door timers when this card is presented.
Panel/Area will UNSET when card is presented at entry reader.
Panel/Area will UNSET when card is presented at exit reader.
Panel/Area will FULLSET when card is presented twice at entry reader.
Panel/Area will FULLSET when card is presented twice at exit reader.
Access a door without PIN on a door connected with PIN pad.
Priority cards will give access when doors are offline.
//4370
Card may allow other cards through doors requiring Escort.
First person to enter the area and the last person to leave.
Delete This Card!
OK
Cancel
No Access
24 Hour
Delete this user's card?
<Unassigned>
//4380
Firmware type not compatible with panel!...
Wireless Only
Loading Calendar Data....
Please select a Calendar...
Access
Paste settings from Door
to Door
Continue?
Paste Door Settings
//4390
View the historical Access log.
!! Language Option not available on 
Access Nodes issue!....
The number of Access nodes in the config file does not match the number
of Access nodes on the panel....
Access nodes on Panel
Access nodes in Config File
Requesting Door
Quick Log - Door
//4400
Date/Time Lost
User RF Panic Button pressed
User Man Down Trasmitter Alarm






//4410
PANEL INFORMATION
PANEL TYPE
FIRMWARE VERSION
SERIAL #
LAST CONFIGURATION TIME
PANEL TIME
ENGINEER MODE
SYSTEM ELECTRICAL CHECKS
BATTERY VOLTAGE
//4420
MAIN PSU VOLTAGE
MAIN PSU CURRENT
MAIN PSU FREQ.
MAINS POWER TEST
BATTERY FAULT TEST
AUXILIARY FUSE
EXTERNAL BELL FUSE
INTERNAL BELL FUSE
BELL TAMPER INPUT
//4430
CABINET TAMPER SWITCH
AUXILIARY TAMPER 1
AUXILIARY TAMPER 2
WIRELESS ANTENNA
WIRELESS JAMMING
MODEM 1
MODEM 1 PHONE LINE
MODEM 2
MODEM 2 PHONE LINE
//4440
CABLE FAULT
FAIL TO COMMUNICATE
USER DURESS
X-BUS DEVICES CHECKS
KEYPAD ID
STATUS CHECK
INPUT STATES CHECK
EXPANDER ID
ZONE/DETECTOR CHECKS
//4450
ZONE ID
SOAKED
INHIBITED/ISOLATED
STATE TEST FAILED
TESTED
FREQUENT USE FAIL
Report Path
Password
Calls to panel allowed
//4460
Romanian
Dutch
Russian
Frequent Time
Hours
Period in which frequently used zones are expected to open at least once when unset
Frequent Use
Get Request Failed
Glass Break
//4470
Cannot find Remote Service database file.... Remote Service will be disabled...
Remote Maintenance
Enable Remote Maintenance
DB Path
Select DB Path...
Remote Maintenance DB
Select Remote Maintenance database to use....
File does not exist!!

//4480
Connected device is not a supported SPC panel type....
Remote Maintenance not available in panel
Profile
Alarm Restores
Tamper Restores
Zone + System alarm restores
Zone + System tamper restores
Mains Fault
Battery Fault
//4490
Alarm Restores
Tamper Restores
Could not find
file
You will need to restart the application for this change to take affect
File
does not exist
Select company logo to appear at top of Maintenance Reports...
Alarm Restore
//4500
Tamper Restore
Failed to retrieve service report from Remote Maintenance database!
Could not update the Report Status in the Remote Maintenance Database!
DOOR CONTROLLERS STATUS/TAMPER CHECK
Date/Time
Report ID
ERROR
A comms failure occurred during the 'Service Maintenance Report' retrieval...
Message Received
//4510
A comms failure occurred during the 'Service Due Date/Time' update...
Report/Update Failed
Remote Maintenance Server Error...
Report corruption error...
Modem connection error...
IP connection error...
Comms transfer error...
Comms Timeout error...
Modem Connection timed out...
//4520
Comms Error
Enable Incoming IP
Allow incoming IP connections...
Incoming IP Port
These parameters are also part of the SPC Pro connection configuration.
Changes made here can also affect the SPC Pro settings....
Incoming IP Connection Settings
Outgoing Modem && IP Connection Settings

/4530
Remote Maintenance ID
Same as
Void Card
Check to temporarily disable this card.
Unset on Entry Reader
Unset on Exit Reader
Full set on Entry Reader
Full set on Exit Reader
Could not read the Installations' Maintenance Report Status from database!
//4540
Remote Maintenance Problem!!
Alert - Remote Maintenance Server has stopped!!!!
Close
Save Settings - Are you sure?
Remote Server Settings
Cannot not find the configuration file!...
Log File
Report/IP Settings
Modem
//4550
System Event Log
File
No Log
Level 1 [Lowest]
Level 2 [Low]
Level 3 [Medium]
Level 4 [High]
Level 5 [Highest]
Errors
//4560
Warnings
Information
All events
Failed to start the Remote Maintenance Database monitoring!
Failed to add a report request to Remote Maintenance database!
Reading list of Reports...
Please Wait....
Failed to read Remote Maintenance Reports from database!
Could not read the Installations' Server Report Status from database!
//4570
Remote Maintenance Service Running...
Remote Maintenance Service Stopped!!
These parameters are also part of the Remote Maintenance configuration.
Changes made here can also affect the Remote Maintenance settings....
Enter authorisation code
Authorisation Required...
Incorrect authorisation code entered!
Auto analyze all 'New' Maintenance Reports?
Maintenance Reports
//4580
Reading list of New Reports...
Please Wait....
Could not read list of new Reports from Remote Maintenance database!
'New' Maintenance Reports found - Analyse now?
Please Wait - Analyzing reports.....
of
Could not get Maintenance Report from database!
Could not update the Report Status in the Remote Maintenance Database!
No New Maintenance Reports found...
//4590
Could not delete the Installation Record from the Remote Maintenance Database
Could not delete the installation's reports from the Remote Maintenance Database
PANEL TYPE ERROR
You have selected to work with an installation with Panel type
This panel type is not supported by this version of
Auto-analyze & status-assign new reports...
Comms Failure Problem
Could not read Maintenance Report status from database!
Could not update installation record in Remote Maintenance Database!
//4600
Failed to modify the Remote Maintenance Server database with updated Service Status!....
Isolated
Inhibited
Alert
Input
YES
NO
Disabled
OK
//4610
No Response
Fault
Bad Pin
Line Fault
Bad SIM
AREA INFORMATION
AREA
LAST SET
LAST UNSET
//4620
LAST ALARM
By User
DOOR CONTROLLER
ARC TESTS
ARC ID
Node was reset!
Node 12V supply low!
Lid is open!
Back tamper is open!
//4630
Battery Fault!
Mains Fault!
Over Current!
RF Jamming detected!
Antenna Tamper!
Node fuse 1 blown!
Node fuse 2 blown!
Node fuse 3 blown!
Node fuse 4 blown!
//4640
Node no longer communicating!
Node cabinet tamper!
Node fuse fault!
Node Mains Fault!
Node Battery Fault!
RF Jamming detected!
Antenna tamper detected!
Panic button is pressed!
PSU Jumper not fitted!
//4650
MODEM
TESTED OK
NOT ENABLED
NO TEST YET DONE
TEST FAILED
MODEM FAILED
Please enter a valid Installation ID!....
Please enter an installation name....
You already have an installation with that ID - please change the ID
//4660
Failed to add installation record to Remote Maintenance Database!
Could not update installation record in Remote Maintenance Database!
Copying firmware file to Fast Programmer
Configure Server Settings...
Use Default
Select New Graphic...
Maintenance Report Letterhead Logo graphic


//4670
Remote Maintenance Server Config...
Modify Remote Maintenance Server Settings...
NOTE : You must restart the Remote Maintenance Service after 
saving these settings for any new changes to take affect...
Add New Modem
Save
Cancel
Destination
File Path
//4680
Log Level
Type of Events to Log
Max Log File Size
Number of panel Events added to report
Allow incoming IP connections from panels
TCP Listen Port
Remove Modem from Config
Modem Port
Pre-listen string
//4690
Post-listen string
Pre-dial string
Pre-dial wait
Enable for incoming calls
Enable for outgoing calls
Loading Calendar Data....
Please select a Calendar...
Reported alarms being restored
Fault Restore
Fault and Tamper restores
Indicate Full Set
Flash 'Red' Indicator light when Fullset. 
Triggers that will Momentarily Unlock Door
Reset Cards
If checked access cards passback state will be reset every day at midnight.
Warning!! - Before performing this upgrade please ensure that your
panel has already been upgraded to the correct new firmware!!


//4710
Reader
Allows Partset A of alarm by SMS
Allows Partset B of alarm by SMS
Allows Clear alerts by SMS
'--- SMS commands that can be sent to panel....
FSET
USET
SSTA
LOG
ENGA
MANA
O
X
ASET
BSET
CLR



//4730
Loading Calendar Data....
Please select a Calendar...
Keyswitch
<None>
Centre Position
Right Position
Left Position
Disabled
System Output
//4740
Area Output
Zone Mapped
Select a door output function....
Select a keyswitch ID....
Edit Holiday
There are Keypad Audio files associated with this panel...
Do you wish to send these files to the panel?
Sending keypad audio files...
Type
//4750
Config Datestamp
Printer Error!... Error connecting to printer....
<No Doors>
Action
Unset
Partset A
Partset B
Fullset
Area Action Trigger
//4760
You have reached the max. number of Area triggers that can be assigned!!
Trigger
Edge
Action
N.B. This is the same number used by SMS Control Configuration. 
Any change made here also affects the SMS Control settings...
N.B. This is the same number used by SMS Event Reporting. 
Any change made here also affects the SMS Event settings...
Failed to retrieve/decompress Maintenance Report!
//4770
DETECTORS FREQUENCY USED TEST
There is no default printer assigned...
Please set up a default printer on this PC...
Compress Data Failed
No Carrier
Modem Connection Failed
Remote Part Closed Connection
Y-modem transfer failed
Could not open Socket connection
//4780
IP Address Wrong
This card has already been assigned to another user!...
Users must be assigned unique cards!!...
Copy/Paste Door Config
Select the Door config items that you wish to copy....
Door Settings
Enable Paste
Zone Settings :
Door Timers / Attributes :
//4790
Calendar Assignments :
Trigger Assignments :
Select the Door configuration settings that you wish to copy....
OK
Cancel
Configure Area Group
Select areas assigned to this group...
Description
Areas assigned to this Area Group
//4800
Add New Area
Delete Group
OK
Cancel
Area Group
You have chosen to remove the Parameter Server Import/Export directory
Are you sure?
Import/Export Directory removed!...
Could not remove Import/Export Directory!...
//4810
Select Configuration Directory
Select configuration directory to use in this session....
An SPC Safe Import/Export directory
has been detected on this PC...
Please choose whether to load the installations found in this
directory or use the normal SPC Pro installations.
Load SPC Safe Import Installations
Ignore Import Installations - Use Default Location
Load Installation data from default location
//4820
Load SPC Safe Import/Export Installations
Cannot find file
Remote Maintenance Service Running...
SPC Pro/SPC Safe
File does not exist!!
Could not load config file!...
Fire
Medical
Dual Keys
//4830
Logo
Analog Clock
Fire Alarm (using 2 soft keys)
Medical Alarm (using 2 soft keys)
Indicate Soft Keys
Show logo in idle mode
Visible in Idle Mode
Disabled
Left Aligned
//4840
Centred
Right Aligned
Centre Position
Right Position
Left Position
Keyswitch
Please enter a password...


//4850
Fire Pre-alarm Time
Period in which a fire alarm is not reported
for zones with 'Fire Pre-alarm' attribute set
Fire Recognition Time
Extra time allowed to see if there is a fire
for zones with 'Fire Pre-alarm' and 'Fire Recognition' attributes set
Coded Restore
Allow user to restore non user alarms using a one time only code.

//4860
Incoming Connection Settings
Outgoing Connection Settings
SPC Pro/SPC Safe
Check to allow SPC Pro/SPC Safe to connect to panel
Check if engineer access must be granted for SPC Pro/SPC Safe to connect
Password used by SPC Pro/SPC Safe
Check to allow SPC Pro/SPC Safe to connect through IP
TCP port panel listens to for incoming connections from SPC Pro/SPC Safe

//4870
Enable Reporting
Reporting Timer
Check to allow the panel to contact the server
after its configuration has been changed
How long after the last configuration change the panel should
contact the server to report its configuration (in minutes)
Server Address
Hostname, URL or IP address of SPC Safe server
Server TCP/IP Port
//4880
TCP port of SPC Safe server
Comfort Keypad
Indicator
Key Switch
Fire Pre-alarm
Fire Recognition
Exit Open
Man Down Test
Unset
//4890
Audio Configuration
Logo Configuration
I/O [0In/0Out]
All zones assigned
some wireless devices may not have zones assigned
<Not Assigned>
Error occurred sending Audio file to panel!...
Max. number of ARCs assigned...
Retrieving Report Data....
//4900
Error occurred retrieving Report...
Loading Report....
Only available when online to panel!...
Assigned
Fullset Common
Fullset common area when all areas fullset
Fullset All
Fullset all areas when common area fullset
Unset Common
//4910
Unset common area when any area unset
Unset All
Unset all areas when common area unset
with Ethernet
Very Low
Panel is not in Engineer Mode!
Access Denied! Manufacturer access required!...
Requesting Event Log for ARC
Event Log
//4920
Problem occurred retrieving ARC Log...
Dial Interval
Period between retrials
Panel Master
Check this to make the panel master of polling messages
Automatic Setting/Unsetting by Trigger(s)
N.B. For Area Auto Set/Unset to occur ALL of the conditions
is one of the triggers must be valid...
Remove Trigger
//4930
Add Trigger
Common Area Settings
Comms Settings - CEI-ABI
Communications - CEI-ABI
CEI-ABI Protocol Settings
Enabled
Check this to enable CEI-ABI support. (Italian firmware only!!!!)
Connection Mode
Client - The panel will connect to the CEI-ABI receiver
//4940
Server - The panel will listen for connections
Server IP Address
TCP/IP Address of CEI-ABI receiver. (Only required in client mode).
Server Port
TCP/IP Port
Physical Address
The control panel's physical CEI-ABI address.
Logical Address
The control panel's logical CEI-ABI address.
//4950
CEI-ABI
Function Keys
Visual Indication
Audible Indication
Limitations
Input
Zone
Active
Zone Text
//4960
Type
Area
Edit
Keypad
Calendar
Mapping Gate
Keyswitch
Keypad
Card Reader
//4970
Disable keys during entry time
LED
Function
ON
OFF
Key
Area
Function
Select if indicator module is located in a secured area.
//4980
Alarms
Select if alarms should be audible.
Entry / Exit
Select if entry and exit should be audible.
Key Press
Select if keypress should be audible.
OK
Delete
Cancel
//4990
Flexible Mode
Linked Mode
NONE
Unset
Partset A
Partset B
Fullset
Toggle Unset/Fullset
Toggle Unset/Partset A
//5000
Toggle Unset/Partset B
Function Keys
Visual Indication
Audible Indication
Deactivation
Areas
Send PC Date/Time to Panel
Reader Type
Automatic Setting/Unsetting by Calendar
//5010
Remote Maintenance ID
Desription
Timer
Add New Mapping Gate
Area Group Configuration
Group ID
Group Description
Areas Assigned
Add Area Group
//5020
Area Groups
Mapping Gate Condition
Select Mapping Gate and state....
Keyswitch Condition
Select Keyswitch and Key Position....
Indicator Condition
Select Indicator and Button number....
None
Button
//5030
Indicator
Button Number
Keyswitch
Key Position
Mapping Gate
State



//5040
Off
Red
Green
Amber
Flash [Slow]
Flash [Medium]
Flash [Fast]
Permanent

//5050
Indicator Expander Output Function
Configure the settings for this indicator output...
Output Function
Assignment
Change
Output State when function is ON/OFF
ON State
OFF State
Colour State
//5060
Flash State
Save
Cancel
Area
Select if keypad is located in a secured area.
Select which areas can be controlled through keypad
Alarms
Entry/Exit
Chime
//5070
Keypress
Voice Annunciation
Fullset
Fullset by pressing function key F2 twice.
Partset A
Partset A by pressing function key F3 twice.
Partset B
Partset B by pressing function key F4 twice.
Direct Set
//5080
Indicate Fullset / Partset function keys
Backlight Intensity
Latch
Select if key position should be latched.
Latch Timer
Enter duration of latch in seconds
(0 - 9999, 0 means latch lasts until key is turned the other way).
Visual Indications
Left
//5090
Right
Output
Copy Door Settings
Paste Door Settings
GPRS Enable
GPRS Address
GPRS Port
Check if events can be reported through GPRS. (Requires GPRS enabled modem)
GPRS Network IP address of receiver.
//5100
GPRS Network UDP port of receiver.
Must match that in SPC Pro
Remove Parameter Server Import/Export directory from PC.
In Linked mode you must assign a keypad!...
LED Always
Select if LED indicators should be active when keys are deactivated
Secure PIN
If checked user PIN code will always be a generated by panel.
Disable SPC Safe
//5110
Enable SPC Safe
German
Lock Supervision
Active only when a valid card/fob is presented to the builtin card reader.
Portuguese
Flemish
Alarm Abort
Problem writing to .INI file!!!.....
Sending peripheral firmware file...
//5120
Peripheral file upload failed!....
Max number of users reached
You cannot add any more users...
Panel region is not supported on this version of SigNETpro!...
File transfer to X-BUS Modules failed
There are no modules connected which support voice annunciation
Firmware version incompatible. Upgrade not allowed!...
License Key is invalid for this panel...
Could not connect to SigNET Fast Programmer....
//5130
This will modify all of the system inputs - Controller AND Expanders....
Are you sure?....
Change System EOL....
Remove this Exception Day from this Calendar?
Centre Position
Right Position
Left Position
Button 1
Button 2
//5140
Button 3
Button 4
Maximum number of allowed Mapping Gates has been reached!....
Value exceeds Max value - Change the Max value parameter
Phone numbers must be 16 digits or less...
Please make a selection from the grid above...
failed
Hardware ID
Device Firmware
//5150
Available Firmware
Device Type
Upgrade
Sending License Key to panel....
License Key accepted!
Error occurred sending license key...
The License Key you entered is not valid for this panel...
Alarm Abort Time
Time after a reported alarm in which an alarm abort message can be reported

(0 = Infinite Timer, 0 - 999)
License Panel (Engineer Mode Only)
Please enter a key in the entry box...
License Key
Enter License Key
Send Key to Panel...
Alarm on Exit Fault
If set then alarm will be raised on exit sequence violations.

//5170
License Panel (Engineer mode only)
Emergency Unset
If checked then Emergency Unset is available.
You have reached the maximum number of WPAs allowed for this panel...
WPAs
Ethernet Protocol
Transport layer protocol over Ethernet.
Call Type
Select the type of call to use when dial-up channel is activated.
//5180
UDP
TCP
Streaming mode
Live video streaming mode.
Disabled
After event
Always
Circuit Switched
GPRS
//5190
Dial-up phone number of receiver.
Backup phone number of receiver.
GPRS Protocol
Select GPRS networking protocol.
Virtual Keypad
Check to allow virtual keypad access from this EDP receiver.
Abort alarm if valid code entered
Early/Late
Early or late setting/unsetting
//5200
Packet Size Limit
Max. packet size for transmission (Default 1440)
Comms Status
EDP commands
A/V Events
A/V Streaming
Keypad use
Log all changes to communication availability.
Log all commands executed through EDP.
//5210
Log when Audio/Video verification events are sent to the receiver.
Log when Audio or Video is live streaming.
Log when virtual keypad is accessed
Generic
Downloading image for Camera
Please select a camera from the list above...
Failed to retrieve camera image...
Camera
Camera Summary
//5220
Refresh Cameras
Show Camera Image
Cameras
MG Output Control
Bypass Unset Delay
WPA Test
Emergency Unset
Video in Browser

//5230
You can select a keypad language for this user that is different
from the language selected for the panel.
If this user enters his/her code at any keypad then
the keypad menus will display in this chosen language.
NOTE: if the panel does not support this user language
then the menus will revert to the default panel language.
Custom
<Same as panel>
Early/Late Setting/Unsetting
//5240
Report Early/Late Setting/Unsetting
Financial
Keypad Language Timeout
Language returns to default language after it is idle for this period (0=Never)
Seismic Sensor Autotest
Average test period for seismic automatic tests.
Automatic sensor Test
Unset Local
Seismic
//5250
Seismic Test
Local Alarm
Door Interlocked
Testing Seismic Sensor for Zone
Seismic test passed!
Seismic test failed...
Audio Expander
Limit Interlocked Door access
Select if the emergency unset code can be entered by pressing '*' key twice.
//5260
Volume Limit
Aux. channel
Max. volume limit for speaker. (0=Disabled)
Check if satellite modules are connected to this expander.
V-Zone
Audio
Video
Camera Type
WPA
//5270
WPA Devices
WPA ID
Name
Transmitter ID
Add New WPA
Add Range of WPAs
WPA Test
Prevent Setting Time
Device Lost Time
//5280
Number of days before notification for untested WPA's. (0 = Test disabled).
If sensor failed to report within this time, then setting will be 
prevented for the area the wireless zone is in, minutes (0 - 720).
If wireless device (sensor or RPA) failed to report within this time,
then it is reported as lost, minutes (20 - 720).
Configure WPA Device - ID
Buttons
Suspicion
WPA Button Functions
//5290
Red
Green
Yellow
Test periodically
WPA Device Name
Tx Device ID Range
There is already a device configured with that Transmitter ID...
Configure WPA Button/Function assignment...

//5300
Add Range of WPA devices...
Enter Transmitter ID Sequence
First ID in sequence
Number of Devices
Last ID in sequence
Select a sequence of Transmitter IDs to configure in a single action...
Cannot create duplicates
There is already a device configured with Transmitter ID
Reading Area Status....
//5310
Peripheral Firmware Upgrade
Upload/Delete Custom Language File
Get Service Report from Panel
File contains the following device firmwares
N.B. : After you send the full firmware file
you may then upgrade individual system devices.
System Devices - Firmware Upgrade
List of EBUS and Modem devices on panel....
List of system devices
//5320
Send new peripheral firmware file to panel....
Upgrade Selected Devices
Close
This feature allows you to upgrade X-Bus device firmware.
You first need to upload the latest firmware version to the panel
and you can then select the X-Bus devices to be upgraded..
A selecção desta norma regional aplicará os requisitos locais ou nacionais que
substituem os requisitos da norma EN50131.

//5330
Area Profile
Disabled
Always
Standard Area
ATM
Vault
Advanced
Not Interlocked
Interlock
//5340
Panic (Silent)
Panic
Duress
You have not selected an Interlock group...
PartSet Options
Linked Areas
Set/Unset
Schedule
Other
//5350
Area Interlock Assignment
Areas assigned to Interlock
area shown in blue...
Area
Description
Assigned Interlock
Configured for this interlock
Interlock
You are attempting to create too many areas....
//5360
Camera Configuration
Configure IP camera settings....
Delete Camera
Are you sure?
Maximum number of allowed Mapping Gates has been reached!....
Redcare/DualCom Type
Output Mapping
Belgium
Austria
//5370
Greece
Cyprus
Israel
Luxembourg
Hungary
Croatia
Serbia
Bulgaria
Bosnia-Herzogovina
//5380
Macedonia
Estonia
Ukraine
Pakistan
Egypt
Kuwait
UAE
Saudi Arabia
South Africa
//5390
Redcare/DualCom
Display System Events
Display Access Events
Custom Language
A custom language file can be sent to the panel...
Custom Language Name on Panel
Custom Language Codepage on Panel
Delete Language File from Panel
Send New Language File to Panel
//5400
none
1250 (Central Europe)
1251 (Cyrillic)
1252 (Latin I)
Could not read Custom Language info from panel...
Sending Custom language file...
UNKNOWN
You are about to download a language file to the panel with the following details
Language Name
//5410
Language Codepage
Continue download?
Custom Language File Download
Setting Prefix
PIN code OR Card
Door must be assigned to a door group.
Error upgrading device...
Firmware Upgrade

//5420
Passed!
Failed!
Pin/Site
All Okay
Verification
Check if Audio/Video verification should be sent to this receiver.
Non-standard SIA
Codes un-supported by SIA standard
Copy file to programmer
//5430
All Files
DHCP Enabled
Trouble
You have exited engineer mode with faults still on panel.
Please review the status screens to determine these panel faults.
Disabled
OK
No Response
Fault
//5440
Bad Pin
Line Fault
Unknown Status
N/A
Ready
Detecting
Initializing
Dialing
Answering
//5450
Connected
Disconnecting
Busy
Linked
Calendar
Triggers
Type


//5460
Area
Active
Text
Entry
Exit
Common
PartSetA
PartSetB
Group ID
//5470
Group Description
Areas
Disabled
Tamper
Trouble
Alarm
Default
Card and PIN
Card or PIN
//5480
System Language
Last Used
Panel is configured for Financial - you cannot disable areas...
PD6662 (EN50131 Grade 2 Based)
PD6662 (EN50131 Grade 3 Based)
EN50131 Grade 2
EN50131 Grade 3
SSF1014:3 Larmclass 1
SSF1014:3 Larmclass 2
//5490
TO-14 (EN50131 Grade 2 Based)
TO-14 (EN50131 Grade 3 Based)
SWISSI Cat 1
SWISSI Cat 2
Max Seismic Test Duration
Time after a reported alarm in which an alarm abort message can be reported
(0=Infinite, 0-120)
RF Output Time
Time the RF output will remain active on system.
//5500
Time Sync Limit
If time within limit then no event will be reported.
Suspicion Audible
If checked then suspicion alert is audible at keypads.
Show Offline Cameras
If checked then offline cameras will be displayed on the keypad in unset mode.
Forbid Setting on Alert
If checked then an area or system cannot be set if there is an area
or system alert present on the system.
//5510
Antimask Set
How antimask is reported when panel is set.
Antimask Unset
How antimask is reported when panel is unset.
Seismic Test on Manual Set
If checked then all seismic sensors in any area that is being set
will be tested before area or system set.
Silence during Audio Verification
If set then the internal and external bells, keypad buzzers, and annunciation
//5520
messages on the MAK will be silenced during audio verification.
Retrigger Duress
If set duress will retrigger.
Retrigger Panic
If set panic will retrigger.
Audio Expander LED
If set audio expander will not turn on led when microphone active.
Engineer Exit
If set the engineer will be allowed to leave with alerts active.
//5530
Idle State Language
Language in which idle state messages are to be displayed.
Door Mode Set
How doors will act when panel is set.
Door Mode Unset
How doors will act when panel is unset.
Override reader LEDs
If set, then the LED behaviour of readers will be controlled by panel.

//5540
Error occurred sending license key...
Advanced Output Config
Latch Output Config
Autoarm Output Config
Entry Time
Fire Exit
Unset
Alarm Reset
Resetting Alarm
//5550
Engineer Exit
On
Keypad
Progressive
Pulse
N.B. At least one option above must be selected.
Output will remain on if autoarm active
Output will follow keypad operation
Output will give progressive warning of autoarm
//5560
Turns on on at end of exit time and off at beginning of entry time
Turns on if any Fire X zones are active
Turns on if user unsets systems, momentary (2s)
Turns on when an alarm is reset , momentary (2s)
Resets during setting procedure if glassbreak /smoke open and not in alarm
Resets when engineer leaves engineer mode, momentary (2s)
Duration autoarm will remain active when pulsed
You must select at least one option for Latch Output function!

//5570
Verification Zone
Save Configuration Summary as file...
RF User Output
Clear All Weeks
Assign to All Weeks
Clear all Week Type assignments from calendar?
Assign Week Type
to all weeks?
WPA Function
//5580
Wireless FOB Panic
Time
Red
Green
Yellow
Red + Green
Red + Yellow
Yellow + Green
Red + Yellow + Green
//5590
Unknown
Any WPA
Function
WPA
Time
KeyFOB Panic
Selected WPA ID and function type....
Time Condition
Select trigger time...
//5600
Wiegand 26 bits
Wiegand 36 bits
HID Corporate 1000
EM4102
Cotag
RF Control
There is already a user assigned to that User ID...
Delay Autoset
Restore Alarms
//5610
Protected
No Video
No Audio
Delete V-Zone
Are you sure?
You have already assigned the max. number of cameras for this panel...
You have already assigned the max. number of V-Zones allowed!...
Settings
Verification Zones
//5620
Cameras
Select Verification zone...
Select Audio file to send...
Getting list of Verification Zones...
Failed to get list of V-Zones...
No Audio available
Audio Online
Audio Offline
Audio file must be at least 1 second in duration...
//5630
There is no audio available for the selected Verification Zone...
The audio test duration time for this selection will be
seconds.
You cannot cancel the test after it has started. - Continue?
The panel has exited Engineer mode. This form will now close...
Connection to panel has been lost. This form will now close...
Sending audio file to panel....
Audio test failed...
Playing audio file at V-Zone
//5640
Recording Audio at panel....
Retrieving captured audio....
Audio retrieval failed...
Confirm that you wish to delete this camera?
Advanced Output
Delayed Setting
RF Output
Modem 1 Line Fault
Modem 1 Failure
//5650
Modem 2 Line Fault
Modem 2 Failure
Battery Low
Entry Status
Warning Status
Error occurred sending file to panel...
Verification
CONTROLLER PSU
WPA DEVICE CHECKS
//5660
WPA Transmitter
CHECK
Battery Status
Supervision Status
Test Status
Last Test
Door Release
Passback violation
Card voided
//5670
Escort required
Custodian required
Invalid PIN
Area is fullset
Door is locked
Invalid card format
Card not on system
Door not authorized for this card
Outside time/date limit
//5680
Card is void
Interlocked door is open
Update area status failed
Error getting Verification data...
Problem deleting file from panel....
Test failed!...
Device filename cannot be recognized
No Custom Language file loaded...
File deletion failed!...
//5690
Virtual Keypad busy...
Un-configured camera...
No image available...
Unable to change mode because of linked area.
Unable to change mode, area is time locked.
Unable to change mode, area is interlocked.
Unable to change mode due to unspecified reason.
Unable to change mode (partset not allowed, or timed, wrong code, etc.
Panel busy.
//5700
You have exited Engineer mode with faults on the system.
Please review the status screens to determine these panel faults.
Areas this user has access to over RF
Key Switch functions
Key
Area
Function
Centre
Right
//5710
Left
Area
Select if indicator module is located in a secured area.
Indications
Outputs
Keyswitch Functions
Event Logging Options
Protocol Version
Select version of EDP protocol to use with this receiver
//5720
Change User Codes
Changing user codes is allowed from this EDP receiver.
GPRS Hangup Timeout
Hangup GPRS call after this time (0=stay connected until IP connection is up).
GPRS Auto Connect
Check if IP network faults automatically triggers a GPRS connection to the server.
Zone States
Zone Input state changes
Network
//5730
IP Network Up/Down events
Duration autoarm will remain active when pulsed
Advanced - Verification Settings
Verification Settings
Audio Settings
Pre-event recording
Post-event recording
Duration of pre-event recording in seconds.
Duration of post-event recording in seconds.
//5740
Verification Zones
Add New Verification Zone
Verification Output Audio Test
Verification Input Audio Test
Cameras
Add Camera
Discover
Verification Zone Configuration
Select A/V sources for this Verification zone....
//5750
Description
Audio
Video
Remove
Save
Close
Verification Audio Output Test
Play test file on verification audio device...
Select Audio File
//5760
Verification Zone
Repeat Count
Volume
Cancel
Play audio via Verification Zone
Select audio file to play on panel...
Select verification zone to play the audio file.
Number of times you want the panel to repeat the audio file.
Volume of output at device.
//5770
[Note: Maximum volume allowed is the maximum volume configured for the device.]
(1 - Max.)
Verification Zone Audio Input Test
Capture and play back audio from verification audio device...
Verification Zone
Recording Duration
Input Volume
Select verification zone to play the audio file.
How long to capture audio (in seconds - max. 30 seconds)
//5780
Volume of input microphone.
Capture Audio Now
Play back captured audio
Close
Add/Edit Camera
Edit configuration details for selected camera...
General Settings
Camera Settings
Searching for Cameras ... Please wait....
//5790
Cancel
Read Camera Settings
Advanced Camera Settings
Camera Snapshot
Send Settings to Camera
Remove
Cancel
Save
Exit Advanced Mode
//5800
Camera ID
Description
Type
Camera IP
Camera Port
Command String
Pre Event Images
Pre Event Interval
Post Event Images
//5810
Post Event Interval
Authentication Enable
Username
Password
Resolution
Camera ID on SPC Panel
Description of camera.
Model of IP Camera
TCP/IP Address of camera.
//5820
TCP/IP Port of camera.
Command to send to camera to get images.
Number of pre-event images to record
Interval between pre-event images, in seconds
Number of post-event images to record
Interval between post-event images, in seconds
Check if Camera Authentication is enabled
Username for IP Camera authentication
Password for IP Camera authentication
//5830
JPEG picture resolution of IP Camera
Cancelling...
Reading camera settings
Failed to communicate with camera.
It is possible a username and password is required.
Insert the administrator username and password below if required by the camera.
WARNING - Camera Comms failure.
Advanced Camera Settings
Add IP Camera
//5840
Edit IP Camera
IP Camera Discovery
Discovery of SPC compatible cameras.
Discovered Cameras
Refresh Devices
Add Camera
Close
Searching for Cameras ... Please wait....
Skip
//5850
No.
Camera Name
IP Address
MAC Address
Model
Configuration
Already Configured
New

//5860
Video Verification - Test
Test camera functionality...
Please Wait...
Show Alarm Pics
Get Snapshot
Trigger Alarm
Close
Video Verification - Snapshot
Snapshot
//5870
ERROR Loading Picture
Warning
Disable Exit Time
Disabled
Triggers
Linked Area Options
Fullset
Fullset All
Prevent Fullset
//5880
Prevent Fulset All
Unset
Unset All
Prevent Unset
Prevent Unset All
Fullset this area when all linked areas fullset.
Fullset all linked areas when this area fullset.
Prevent this area from Fullset if any linked areas are Unset.
Prevent linked areas from Fullset if this area is not Fullset.
//5890
Unset this area when any linked area unset.
Unset all linked areas when this area unset.
Prevent this area from Unset if any linked areas are Fullset.
Prevent linked areas from Unset if this area is Fullset.
Linked Areas (select which areas are linked to this area)
Setting/Unsetting Options
Setting/Unsetting
Warning Time
User Cancel
//5900
User Delay
Keyswitch
Delay Interval
Delay Limit
Dual Code
Delayed Unset
Unset Duration
Interlock
Note: this setting applies to automatic Calendar setting and Timed Unset.
//5910
Number of minutes to display warning before fullset.
Select if setting can be cancelled by entering user code on keypads.
Select if setting can be delayed by entering user code on keypads.
Select if setting can be delayed by using a keyswitch module
The number of minutes setting is delayed.
The number of times setting can be delayed. [0 = unlimited]
Select if/when two valid user codes are required to Set/Unset.
Delay time in minutes for delayed Unset, leave at zero for no delay.
If area is unset for longer than this period, then area will set automatically. 
//5920
0 means not active.
Select if area should be interlocked. 
(Access is prevented if other interlocked areas of the same type are Unset.)
View Areas in selected Interlock
Schedule (Calendar Set/Unset)
Scheduler
Unset
Fullset
Time Locked
//5930
Vault Access Timer
Reporting
Early to Set
Late to Set
Earl to Unset
Late to Unset
Panel can be configured to report to CS if it is Set or Unset outside
of the normal scheduled calendar times.
Enabled
//5940
Timer
View Selected Calendar Settings
Create New Calendar
Mins.
Select if area should automatically unset according to calendar.
Select if area should automatically fullset according to calendar.
Select if area should be time locked according to calendar.
This timer is activated at the start of a Time Locked unset period.
If the area is not unset when this timer expires then
//5950
the area cannot be unset until the start of the next Time Lock unset period.
(0 means not active.)
Report if manual fullset before the scheduled fullset (minus timer).
Report if area that is not fullset at scheduled time (plus timer).
Report if manual unset before the scheduled unset (minus timer).
Report if area that is not unset at scheduled time (plus timer).
Other
Entry/Exit
'All Okay' required
//5960
'All Okay' verification Time
'All Okay' event
Fob Unset Entry
RF Output
RF output Time
User must confirm 'All okay' input, or silent alarm will be generated
Time (seconds) in which 'All okay' must be confirmed before alarm is raised
When All okay timer expires which action should be taken
FOB will only unset when the entry timer running
//5970
How long will output remain on (Seconds), 0 = toggle
Searching for CCIC1410 Cameras
Searching for CFMC1315 Cameras
Quick-Configure Vault/ATM Areas
Quick Configuration Utility for Vault / ATM Areas
Select details for Vault/ATM type Areas on system....
Configure Vaults
Configure ATMs
Number of Vaults
//5980
Link Vaults
View/Edit Defaults
Number of ATMs
Link ATMs
View/Edit Defaults
Defaults
Enabled
Check this box if you want these new Vault areas to be linked together.
Edit the default settings that will be applied to each new Vault areas.
//5990
Check this box if you want these new ATM areas to be linked together.
Edit the default settings that will be applied to each new ATM areas.
Create Vaults/ATM areas now
Close
This Quick-Configuration utility allows you to generate a group of Vault
and/or ATM areas with matching defaults. This utility is normally used
to create Vault and/or ATM areas for a new clean installation with no
Vaults or ATMs yet created.
Enable Partset
//6000
Area Trigger Settings
Configure Trigger Arming for the System...
Automatic Setting/Unsetting by Trigger(s)
Remove Trigger
Add Trigger
N.B. Auto Set/Unset will occur when ALL conditions in a trigger are valid...
Close
Test Channel
Channel Test Failed...
//6010
Upgrade to
Custom Language Codepage
Central Europe
Latin
Import SPC Pro Language File
Pace
WPA Only
N.B. If secure area is set to 'NONE' exit entry will not operate on this keypad.
Allow custom language selection on supported panels....
//6020
Delay Fullset
If checked the exit timers are used across all areas.
Select for compliance to Swedish requirements
Select for compliance to Belgium (*) requirements
Select for compliance to Swiss (*) requirements
Card Added
Card Deleted
Card Reset
Card Attribute Changed
//6030
Invalid Format
Unsupported country
hh:mm
Partset Buzzer
Enabling will sound exit timer during Partset
Detector Fault
Holdup Fault
Warning Fault

//6040
Confirmation Zones
No of zones alarms required in a single area to trigger a confirmed alarm
Checking all parameters
Defaulting Camera
Waiting for camera to resume from reset
Restoring network settings
Resetting Camera
Waiting for camera to resume from reset
Downloading settings to camera
//6050
Resetting Camera
Waiting for camera to resume from reset
Reading settings back from camera
Closing
Send Settings to Camera
Send and save the settings to the online camera....
Default Camera
Default camera to a suitable configuration before sending new settings.
Note that with this option the camera user name and password will be reset.
//6060
Searching for cameras...
Warning: advanced settings is provided by a direct connection to the
camera via a browser. Changes made in the advanced screen will not be
saved to the panel configuration file.
Click OK to proceed or Cancel to return to standard configuration.
Warning - Advanced settings.
SPC Pro will launch your default browser to connect to this camera.
Advanced Options
There was an error when trying to open a default browser
//6070
Miscellaneous
'Redcare' modem option is only applicable to panel HW Version 2
Select for compliance to Spanish requirements
Daily trigger time (hh:mm)
Report IP Network Up/Down events
Network
Card voided at the keypad
Invalid Format
Incorrect Site Code
//6080
Clock Data Reversed
Void Card
Unknown Card
Please enter a description before saving...
Encryption key must be 32 characters in length!




//6090
Edit user settings, profiles, etc.
Duress Enable
NOTE: This is a Global User - Edit/Delete is not possible!!...
Date Limit
Enabled
to
User Profiles
Check to enable duress codes for this user...
Card Number
//6100
Enter card number.
Access Control
SMS Setup
WEB Password
Configured
Configure SMS settings
Configure Web Password
User Profile
View selected profile settings
//6110
Create new profile
Edit User Profile
Edit the permissions, rights, areas for this profile...
Panel Rights for this profile
Areas this profile has access to
User Profile ID
User Profile Name
Calendar
Access Control
//6120
Site Code
Site code of all cards using this user profile
NOTE: This is a Global Profile - Edit/Delete is not possible!!...
User Profile Name
User Profile List
User Profiles used to determine a user's permissions, rights, etc.
Add New User Profile
Close
Are you sure you want to delete this user profile?
//6130
Please enter a profile name
Events Enabled
Control Enabled
Card formats
Select supported card formats
Set Users
Set Users master
Set User Profiles
Set Calendars
//6140
Set Doors
Global
Duress User
User who caused duress
Duress Location
Location duress occurred in
Last Duress Time
Time of last duress event
Restore Zone
//6150
Report in Eng mode
When in engineer mode, panel still reports alarms, panics, etc.
Last Late to Set time
Last Late to Unset time
Last Fail to Set time
Not ready to set
Not ready to unset
Last alarm abort time
Restore Zone
//6160
NOTE: This is a Global Calendar - Edit/Delete is not possible!!...
NOTE: This is a Global Exception Day - Edit/Delete is not possible!!...
SPC Manager
Mode
Disabled
6 PIN Digits
7 PIN Digits
8 PIN Digits
SPC Manager global-user mode
//6170
Upgrade process
Some items may need to be reprogrammed after upgrade.
Maximum number of profiles reached
No Profile Selected
You must assign a user profile!...
There is already a user with that name!
Cannot delete a profile that is in use!...
Delete profile ID
Seismic Test
//6180
Set Users [Master]
Set User Profiles
Set Calendars
Set Doors
View Profile Usage
You must enter a phone number!...
Delete User SMS
User list for Profile ID
List of users assigned selected profile...
//6190
Report in Eng Mode
The panel will always report alarm activatations, panics alarms
Card Formats
Select supported card formats on access control system
SPC Manager Enable/Disable
Max number of SMS entries reached - you can't add any more...
Delete Web Password
User SMS
User Web Passwords
//6200
Card Number
Profile
Add SMS
SMS ID
SMS Number
User SMS Configuration
Configure SMS settings for this user...
Profile name
Add profile
//6210
Select languages to support...
Setting Authorisation
Lock Element
Please enter a valid card number!...
You already have a user with that card number!
Panel Rights for this profile
Areas this profile has access to
User Profile ID
User Profile Name
//6220
Calendar
Access Control
Site Code
Site code of all cards using this user profile
NOTE: This is a Global Profile - Edit/Delete is not possible!!...
Seismic Test
Set Users [Master]
Set User Profiles
Set Calendars
//6230
Set Doors
View Profile Usage
You must enter a phone number!...
Delete User SMS
Enable SPC Manager
Mode
WARNING!!! - User codes may need to be adjusted!...
Disabled

//6240
Enable - 6 PIN Digits
Enable - 7 PIN Digits
Enable - 8 PIN Digits
You already have a user with that name!
Wiegand 26bit
Wiegand 36bit
HID Corporate 1000
EM4102
Cotag
//6250
HID 37
HID 37F
HID 37BCD
AR618 WIE BCD 52
AR618 OMRON 80
HID ICLASS MIFARE
HID ICLASS DESFIRE
Wiegand

//6260
User List for Profile ID
List of users assigned selected profile...
Sending language file...
PIN Code Policy
Periodic change required
Warn if changes required
User Selects the last digit
User Selects the 2 digits
Limit Changes
//6270
Secure PIN
You must select a region and grade for this installation..
Select Region...
U.K.
Ireland
E.U.
Sweden
Switzerland
Belgium
//6280
Spain
Germany
France
Unrestricted
VDS Class A
VDS Class C
NF Type 2
NF Type 3
Degrees (C)
//6290
PIN Valid
Period for which pin is valid
Pin Changes Limit
Changes
Number of changes within a valid period
Pin Warning
Time before pin expiry after which a warning will be displayed
Lockout post alarm
Duration after alarm that access will be denied
//6300
Link timeout
Timeout for ethernet link fault (0 = Disabled)
Setting Authorisation
Period setting authorisation is valid for
Camera Offline
Time for camera to to offline
Report in Eng mode
The panel will always report alarm activatations, panics alarms
Card Formats
//6310
Select supported card formats on access control system
PIN Policy
Configure Pin policy
Watchdog Output Mode
Mode of the watchdog output. If enabled, output 6 is used as a watchdog output.
If disabled, output 6 operates as a normal output as configured in the outputs section.
Alarm on reporting fail
If a fail to communicate alert is raised external bells will activate
VDS
//6320
Enable Vds Power Supply
SPC Manager Enable/Disable
SPC Manager Mode
Disable
Enabled
Pulsed
Enabled Inverted
Select for compliance to German requirements
Select for compliance to French requirements
//6330
Not Enabled
Timeout
Socket Invalid
Image Too Small
Buffer Too Small
LFRC Not Found
TCP Abort
UNKNOWN
Memory Issue
//6340
Bad Request
Client Error
Authentication Fail
Max number of SMS entries reached - you can't add any more...
Delete Web Password for User
Delete Web Password
Maximum number of profiles reached...
User Profiles
User SMS
//6350
User Web Passwords
Card Number
Profile
Global
Add SMS
Delete Web Password
Engineer Configure
Copy data and paste data are the same!

//6360
Card not on system
Lock out post alarm
Unknown
Failed due to lack of authorisation.
Failed - not allowed at this time.
PSU
None
Smart PSU
VDS PSU
//6370
PIR 1k/1k/2k2
PIR 4k7/4k7/2k2
Single 1K5
Single 10k
Single 12k
Dual 2k2/4k7
Dual 2k2/1k5
Dual 2k2/1k0
Dual Glass
//6380
Dual 2k2/10k
Edit PSU Output
PSU Link
PSU Out Tamper
PSU Low Voltage
Glass Break
Dual 10k/10k
Force Set

//6390
Ready to Set
Setting Complete
Setting Success
Blockschloss 1
Blockschloss 2
Lock Element Lock
Lock Element Unlock
PIN Tamper
Trouble
//6400
Ethernet Link Fault
Network Fault
Paste settings from Profile
to Profile
Continue
Paste Profile Settings
PSU Type
Refresh PSU Outputs
Primary Battery Only
//6410
Select Supported Card Formats
Monitor Outputs
Test Outputs
Output Monitor
VdS 2471 Compatible
Enforces EDP Receiver settings to meet the VdS 2471 standard
Generate Network Fault
A polling failure will generate a network fault.

//6420
Entry Reader Area
Exit Reader Area
Area on door side :Entry
Area on door side :Exit
No Bells
Access denied on alarm
Access will be temporary denied after alarm
Prevent Setting
Prevent Setting from Keypad
//6430
Prevent Unsetting
Prevent Unsetting from Keypad
Setting Authorization
Setting authorization operation for this area
Authorise Setting
Authorise Setting for linked areas
User Web Passwords
User SMS
User Profiles
//6440
Add Profile
ID
Profile Name
Global
SMS ID
User ID
User Name
SMS Number
Events Enabled
//6450
Control Enabled
WEBPass ID
Mask_1k_1k_6k8
Mask_1k_1k_2k2
Mask_4k7_4k7_2k2
Actuated
Out of Bounds
Unstable

//6460
Initialising
N/A
Charging
Fully Charged
Battery Only
Deep Discharge
Unknown
OK
Fault
//6470
Low
Engineer Auto Log-out
Engineer will be automatically logged out
Out of Bounds EOL Set
How system will react to a zone outside EOL bands when area/system set
Out of Bounds EOL Unset
How system will react to a zone outside EOL bands when area/system unset
Zone Unstable Set
How system should react to an unstable zone when area/system set
//6480
Zone Unstable Unset
How system should react to an unstable zone when area/system unset
EOL Wide
EOLs will use wide bands
Reader Locked
Invalid Code Learning
PIN Expired
Engineer access is denied by panel.

//6490
PSU Status
Mains status
Temperature
Load Voltage
Load current
Charge status
Primary Circuit
Charge Circuit
NF Output
//6500
PSU Output
Status for PSU connected to EnetNode....
Phone number SMS messages will be sent to / received from
SMS Authentication PIN (leave blank to leave unchanged)
Access control door events
Report if Setting/Unsetting is not according to schedule
Valid user code entered on keypad and fire zone active
No DRS
Code Tamper
//6510
Peripheral Firmware
panel may now reset!
Link
Enabled + Reporting (10 sec)
Enabled + Reporting (60 sec)
Unsetting
Display Test message at
Setting
Setting and Unsetting